- Top
- Viewfinder
- Viewfinder status display
- Status display

# Status display

Refer to “Status display (STATUS) in the <MON OUT1>, <MON OUT2>, and <VF SDI> outputs.”.

## Adjusting the screen

Press the <EVF MENU> button.

Screen adjustment items are displayed on the upper part of the screen.

Turn the jog dial button to select the items you want to adjust.

Press the jog dial button.

Turn the jog dial button to make adjustments.

Press the jog dial button.

Press the <EVF MENU> button.

The screen adjustment items display disappears.

This can also be done in [EVF MENU] → [DISPLAY SETUP].

## Direct camera settings

The following camera settings can be set directly through viewfinder operation.

[FPS]/[SHUTTER]/[EI]/[WB]

Press the <CAM MENU> button of the viewfinder.

Setting items are displayed on the lower part of the screen.

Turn the jog dial button to select the items you want to set.

Press the jog dial button.

Turn the jog dial button to select setting details.

Press the <CAM MENU> button.

## [MENU] settings from the viewfinder

The camera’s [MENU] can be directly configured through viewfinder operation.

Press and hold the <CAM MENU> button of the viewfinder for at least two seconds.

The camera [MENU] is displayed.

[MENU] is also displayed on the camera’s operation panel.

## [EVF MENU] operation

Press and hold the <EVF MENU> button for at least two seconds.

[EVF MENU] is displayed.

## [EVF MENU] list

#### [DISPLAY SETUP]

Item | Description of settings
--- | ---
[CONTRAST] | Adjusts the contrast. [−32]…[31] Factory setting: [0]
[BRIGHT] | Adjusts the brightness. [−32]…[31] Factory setting: [0]
[COLOR] | Adjusts the color level. [−32]…[31] Factory setting: [0]
[-- PEAKING VALUE] | Adjusts the outline of the image in the viewfinder. [0]…[9] Factory setting: [0]
[R BRT] | Adjusts the red color brightness. [−32]…[31] Factory setting: [0]
[G BRT] | Adjusts the green color brightness. [−32]…[31] Factory setting: [0]
[B BRT] | Adjusts the blue color brightness. [−32]…[31] Factory setting: [0]

#### [SW MODE]

Item | Description of settings
--- | ---
[FRONT TALLY] | Enables/disables the front tally lamp function. [ON]/[OFF]
[EYE SENSOR] | Sets sensitivity of eye sensor. [NORMAL]: Displays the viewfinder screen according to the eye sensor. [1min]: Keeps the viewfinder screen display for one minute after the eye sensor is released. [5min]: Keeps the viewfinder screen display for five minutes after the eye sensor is released.
[B/W] | Switches to monochrome mode. [ON]: Display will be all black and white. [OFF]: Disables the monochrome mode.
[SCAN] | Reverses the display. [NORMAL]/[REVERSE]

#### [USER SW 1]/[USER SW 2]

Selects the function assigned to the <EVF USER 1>/<EVF USER 2> button.

The setting will be common with the contents displayed and set in the VF related item in [MENU] → [OUTPUT SETTINGS] of the camera.

(excluding [FALSE COLOR])

Description of settings
[MARKER]: Displays/hides markers. [CENTER MARKER]: Displays/hides the center marker. [SAFETY MARKER]: Switches the display/hide of the safety marker. [FRAME MARK]: Displays/hides the frame marker. [USER BOX]: Displays/hides the user box. [ZEBRA]: Displays/hides the zebra display. [EXPAND]: Enables/disables the display enlargement function. [FOCUS ASSIST]: Enables/disables the focus assist function. [IN COLOR/SQ./MONO]: Enables/disables the advanced assist (focus assist) function. [FALSE COLOR]: Enables/disables false color mode. [SURROUND VIEW]: Enables/disables the surround view function. [SURROUND VIEW LINE]: Displays/hides the surround view area marker display. [SMOOTH MODE]: Enables/disables the smooth mode. [WFM]: Displays/hides waveform monitor.

#### [INFORMATION]

Item | Description of settings
--- | ---
[OPERATION TIME] | Displays the total display time of the organic EL panel of the viewfinder.
[VERSION] | Displays the firmware version of the viewfinder.

## False color mode

Check the exposure using the false color.

Image will be displayed with colors sored by luminosity signals. Images of other levels are displayed in black and white.

The false color can be displayed in the viewfinder and the output image from the <VF SDI> terminal.

### Display patterns

#### When [MAIN COLOR] is [V-Log]

Color | Level | Description
--- | --- | ---
(Red) | (White clip −3%) or more* | White-level clip
(Yellow) | (White clip −6%) to (White clip −3%)* | Lower area of the white-level clip
(Pink) | 48.7% - 51.8% | One-stopover color from neutral gray
(Green) | 40.5% - 43.6% | 18% gray neutral color
(Blue) | 10.3% - 13.2% | Upper area of the black-level clip
(Purple) | 7.3% - 10.3% | Black-level clip

The white clip level will differ depending on the [ON]/[OFF] of [EI] and [HIGH SPEED].

#### When [MAIN COLOR] is not [V-Log]

Color | Level | Description
--- | --- | ---
(Red) | (White clip −1%) or more* | White-level clip
(Yellow) | 98% - 100% | 100% level of video output
(Blue) | 2.5% - 4.0% | Upper area of the black-level clip
(Purple) | 0% - 2.5% | Black-level clip

The white clip level will differ depending on the [ON]/[OFF] of [EI] and [HIGH SPEED]. The white clip level for [3D LUT] will be the same level as for [V-709].

Top of the page