- Top
- Video Recording and Color Grading
- Dual-recording
- File name style

# File name style

The file name style for recorded clips can be set in [MENU] → [REC SETTINGS] → [FILE NAME STYLE].

#### [P2]

Start recording

Stop recording

Example: [AVC-Intra4K 422]

[MAIN CODEC]

File name with information split

Example: [AVC-Intra100]

[SUB CODEC]

Fig. 1

Fig. 2

If the file name style is set to [P2], the information split is included in the file name even if the file is separated by 4 GB. (Fig. 1)

The file can be handled as a single clip in editing software, etc.

In the following cases, the file is split by 4 GB and it is recorded as the P2 file name style.

- When the format of the recording media is FAT32

  Recording media | Format
  --- | ---
  P2 | FAT32
  microP2 (32 GB) | FAT32

- When the recording format is OP-Atom format

  [MAIN CODEC] | Format
  --- | ---
  [AVC-Intra200] | OP-Atom
  [AVC-Intra100] | OP-Atom

In the following cases, “M” to indicate metadata is displayed next to the REEL number in the HOME screen and the clip number icon. (Fig. 2)

- Set the [FILE NAME STYLE] to [P2]

- Set the [User Clip Name] to [TYPE3]

#### [CINE]

Start recording

Stop recording

Example: [AVC-Intra4K 422]

[MAIN CODEC]

The file name is the same

Example: [AVC-Intra422]

[SUB CODEC]

Fig. 1

Fig. 2

1. CAM INDEX

2. REEL No.

3. Clip number

4. Date

5. Hashtag generated from the serial number of the recording module

The [CINE] setting of the file name style is enabled if the following conditions (where a clip is not split by 4 GB) are met.

When these conditions are not met, the setting of the file name style is forcibly switched to [P2] even if [CINE] is set in [FILE NAME STYLE]. An alert is displayed. Check the alert.

- When the format of the recording media is exFAT

  Recording media | Format
  --- | ---
  expressP2 | exFAT
  microP2 (64 GB) | exFAT

- When the recording format is OP-1b format

  [MAIN CODEC] | Format
  --- | ---
  [AVC-Intra4K 444] | OP-1b
  [AVC-Intra4K 422] | OP-1b
  [AVC-Intra4K-LT] | OP-1b
  [AVC-Intra2K 444] | OP-1b
  [AVC-Intra2K 422] | OP-1b
  [AVC-Intra444] | OP-1b
  [AVC-Intra422] | OP-1b
  [ProRes 4444 XQ] | OP-1b
  [ProRes 4444] | OP-1b
  [ProRes 422 HQ] | OP-1b
  [ProRes 422] | OP-1b
  [ProRes 422 LT] | OP-1b

The following happens when [CINE] is enabled.

- The file name of the main recorder and sub recorder is the same. (Fig. 1)

- Recording across slots cannot be performed.

- Recording stops if there is no more space on the sub recorder card even if space remains on the main recorder card.

- “F” to indicate the file is displayed next to the REEL number of the HOME screen and the clip number icon. (Fig. 2)

Even when [P2] is set, the [CINE] file name style (1-5) is recorded in the metadata as [USER CLIP NAME] if [USER CLIP NAME] is set to [TYPE3].

Top of the page