- Top
- Preparation
- Power supply
- Mounting and setting battery

# Mounting and setting battery

## Using Anton/Bauer batteries

Release lever

Anton/Bauer batteries

Mount the Anton/Bauer battery.

Insert the battery terminal and slide in the direction of the arrow.

Set the battery type.

From [MENU] → [SYSTEM SETTINGS] → [BATTERY] → [BATTERY SELECT], select the battery type.

For details, refer to “Setting menu basic operations”.

NOTE

- To remove the battery, keep the release lever of the battery holder completely down, slide the battery in the opposite direction when you mounted it.

## Using V-mount type batteries

Mount the V-mount type battery plate. As shown in the illustration, insert and slide in the direction of the arrow.

Release lever

Mount the V-mount type battery plate.

Slide in the direction of the arrow.

Set the battery type.

- From [MENU] → [SYSTEM SETTINGS] → [BATTERY] → [BATTERY SELECT], select the battery type.

NOTE

- Contact your dealer for information about the V-mount type battery plate.

- When the V-mount type battery plate is used, % (percent) is not displayed even if batteries with a battery level indicator function are used.

- When removing the plate, remove by sliding the release lever.

- When using a battery that is not included in [BATTERY SELECT], set [other], then set [FULL Volt], [NEAR END Volt], or [END Volt] according to the characteristics of the battery.

Top of the page