- Top
- Extension module
- Specifications
- Specifications

# Specifications

## General

Power DC 12 V (11.0 V - 17.0 V) Power consumption 33 W (body only) 63 W (with all optional accessories connected and maximum power supplied from each output terminal)

indicates safety items.

Ambient operating temperature | 0 °C - 40 °C (32 °F - 104 °F)
Ambient operating humidity | 10% - 85% (no condensation)
Storage temperature | −20 °C - 60 °C (−4 °F - 140 °F)
Weight | Camera extension module: Approx. 0.95 kg (2.09 lbs.) Recording extension module: Approx. 0.65 kg (1.43 lbs.)
Dimensions (W×H×D) | Camera extension module: 121 mm×143 mm×73 mm (4-25/32 inches×5-21/32 inches×2-7/8 inches) Recording extension module: 106 mm×143 mm×61 mm (4-3/16 inches×5-21/32 inches×2-13/32 inches)

- Make sure that the total current from the <DC OUT> terminal, <VF> terminal, and <LENS> terminal of the camera module (optional), and the <DC OUT> terminal of the camera extension module does not exceed 30 W.

Top of the page