- Top
- Video Recording and Color Grading
- In-camera grading
- Grading function

# Grading function

[CDL]:

- Controlled using [Slope], [Offset], [Power] (RGB stand-alone), and [Saturation] (RGB common).

- Can be controlled in real-time using the camera’s control panel.

- Control parameters are saved to a file and stored in a P2 card together with videos, etc.

  It can also be saved to the SD memory card.

- The file extension is .cdl.

[3D LUT]:

- Controlled in a 17-grid [3D LUT] file.

- Uploads data within the camera through an SD memory card.

  It can also be saved to the SD memory card.

- Control parameters are saved to a file and stored in a P2 card together with videos, etc.

- The file extension is .vlt.

Top of the page