- Top
- Description of Parts
- Recording module
- Rear

# Rear

1. Battery holder

   For mounting Anton/Bauer batteries.

2. Battery release lever

   Pull this battery release lever down to release the battery.

3. Battery contact terminals

   Contact terminals for the battery.

4. Speaker

   EE audio can be monitored during recording while playback audio can be monitored during playback.

   The alarm is output in sync with flashing/lighting of the warning indicator.

   Audio from the speaker automatically is turned off when headphones are connected to the <PHONES> terminal.

5. <AUDIO IN 1>/<AUDIO IN 2> terminal

   Connect the audio equipment or the microphone.

6. <LINE>/<MIC> switch

   Switch for switching audio input signals connected to the <AUDIO IN 1>/<AUDIO IN 2> terminal.

   <LINE>: Select when audio equipment is connected by the line input.

   <MIC>: Select when a microphone is connected.

7. <PHONES> terminal

   Connecting terminal of headphones for audio monitor. (Stereo mini jack)

8. <DC OUT/RS> terminal

   Terminal for DC 12 V output and REC trigger input. The DC output provides a maximum current of 1.0 A.

9. <DC IN> terminal

   Input terminal for connecting an external DC power supply.

10. <LIGHT CONTROL> switch

    Control switch when light is connected to the light output terminal.

Top of the page