- Top
- Video Recording and Color Grading
- Dual-recording

# Dual-recording

The camera has two built-in recorders.

Sub slot

Main slot

#### Main recorder

Card slot | expressP2 memory card slot × 2
Compatible memory cards | expressP2 memory card P2 memory card (with some restrictions)

- P2 memory cards cannot be used when the 4K format, the ProRes format, [AVC-Intra2K 444] format, [AVC-Intra444] format, [AVC-Intra200] format, or the variable frame rate function is enabled.

- P2 memory cards of 2 GB cannot be used.

- R, A, and E series P2 memory cards cannot be used for 1080/59.94P and 1080/50P.

#### Sub recorder

Card slot | microP2 memory card slot × 2
Compatible memory cards | microP2 memory card

- Proxy data can be recorded simultaneously in the sub recorder (with some restrictions)

- Sub recorder has two types of operation modes. Set the mode using [MENU] → [SYSTEM SETTINGS] → [SYSTEM MODE] → [VFR SUB REC].

  - [NORMAL+Audio]: Records in the frame of system frequency. Audio signal is also recorded.

  - [VFR up to 60p (50p)]: Records in a variable frame rate by synchronizing to the [VFR] setting of the main recorder. Audio signal is not recorded when [VFR] is set to [ON].

  If either of the following is set, the operation mode is fixed to [NORMAL+Audio].

  - [HIGH SPEED]: [ON (1-fps)]

  - [SUB CODEC]: [AVC-LongG50] or [AVC-LongG25]

- Recording using only the sub recorder is not possible.

File name style
Top of the page