- Top
- Description of Parts
- Camera module
- Left side

# Left side

1. Lens flange back adjustment hole

   Used when adjusting the lens flange back.

2. USER buttons (<1>/<2>/<3>)

   User-selected functions can be assigned to each button. Pressing a button performs the assigned function.

3. Focus hook/focus mark < >

   Indicate the focal plane of the MOS sensor.

4. <REC> button

   Press this button to start recording. Press this button again to stop recording. The button lights up in red during recording.

5. <SHUTTER> switch

   Switch for changing the electronic shutter.

6. <EI> switch

   Switch for changing the EXPOSURE INDEX (gain).

7. Accessory mounting holes

   For attaching accessories.

   - Mounting hole size

     - 3/8-16 UNC

8. Handle

9. <LOCK> switch

   Disables the operation of the camera module buttons and switches. (except the <REC> button)

   Keep this in the <LOCK> position to prevent incorrect operation when moving the camera, etc.

10. <WB> switch

    Switch for changing the white balance.

11. Fan inlet

    Fan inlet for dissipating heat. Do not block this when the camera is in use.

Top of the page