- Top
- Menu Operations
- Menu list
- [PERIPHERAL]

# [PERIPHERAL]

Applies settings related to functions used in conjunction with peripheral devices, such as network and GPS devices.

Item | Description of settings
--- | ---
[GPS] | Configures internal GPS settings. [ON]: Activates the GPS operation. Outputs the location information as a signal to the <SDI OUT> terminal and records it as clip metadata. [OFF]: Does not activate the GPS operation. Does not output and record the location information. Factory setting: [OFF]
[NETWORK SEL] | Sets the connection method when connecting the camera with an external device (such as a computer) via network. [LAN]: Connects via the <LAN> terminal. [WLAN]: Connects via wireless LAN. [OFF]: Does not connect. Factory setting: [OFF]
[NETWORK FUNC] | [USER ACCOUNT] | Sets the user account to be used for authentication in the network function of the camera.
| [ACCOUNT LIST] | Displays the currently set account name. Also registers new accounts and deletes accounts.
[LAN PROPERTY] | [MAC ADDRESS] | Displays the MAC address of the <LAN> terminal on the camera. (Cannot be changed.)
| [DHCP] | Sets whether to use automatic acquisition via DHCP. (Mutually exclusive with [DHCP SERVER] setting) [ENABLE]: Uses automatic acquisition. [DISABLE]: Does not use automatic acquisition. Set [IP ADDRESS], [SUBNET MASK], [DEFAULT GATEWAY], [PRIMARY DNS], and [SECONDARY DNS]. Factory setting: [ENABLE]
| [IP ADDRESS] | Sets the IP address when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.1]
| [SUBNET MASK] | Sets the subnet mask when [DISABLE] is selected in [DHCP]. Factory setting: [255.255.255.0]
| [DEFAULT GATEWAY] | Sets the default gateway when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.254]
| [PRIMARY DNS] | Sets the primary DNS server when [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [SECONDARY DNS] | Sets the secondary DNS server when [DISABLE] is selected in [DHCP]. Factory setting: [0.0.0.0]
| [DHCP SERVER] | Sets whether to use the DHCP SERVER function when connected via wired LAN. (Mutually exclusive with [DHCP] setting) [ENABLE]: Uses the DHCP SERVER function. [DISABLE]: Does not use the DHCP SERVER function. Factory setting: [DISABLE]
[WIRELESS PROPERTY] | [MAC ADDRESS] | Displays the MAC address of the wireless LAN of the camera. (Cannot be changed.)
| [TYPE] | Sets the connection method. [DIRECT]: Accesses to the network function of the camera directly from a smartphone, tablet, or computer. [INFRA]: Connects to the wireless access point. Factory setting: [DIRECT]
| [SSID INPUT MODE] | Sets the setting method of SSID. When [TYPE] in [WIRELESS PROPERTY] is set to [INFRA], this item can be set. [SELECT]: Selects the setting from the access point list. [MANUAL]: Enters the setting manually. Factory setting: [SELECT]
| [SSID] | Displays network name (SSID). Factory setting: [AU-VREC1]
| [BAND] | Switches between two transmission methods (2.4 GHz or 5 GHz). [2.4GHz], [5GHz] Factory setting: [2.4GHz]
| [CHANNEL(2.4GHz)] | Sets the channels to be used when [DIRECT] is selected in [TYPE], [2.4GHz] is selected in [BAND], and the camera is connected via wireless LAN. [AUTO], [CH1], [CH6], [CH11] Factory setting: [AUTO]
| [CHANNEL(5GHz)] | Sets the channels to be used when [DIRECT] is selected in [TYPE], [5GHz] is selected in [BAND], and the camera is connected via wireless LAN. The selection differs depending on the installed wireless module. [AUTO], [CH36], [CH40], [CH44], [CH48], [CH149], [CH153], [CH157], [CH161], [CH165] Factory setting: [AUTO]
| [ENCRYPTION] | Sets the encryption format. [WPA-TKIP], [WPA-AES], [WPA2-TKIP], [WPA2-AES], [NONE] Factory setting: [WPA2-AES]
| [ENCRYPT KEY] | Sets the encryption key. Set the key using a string of 8 to 63 characters or a hexadecimal number with 64 digits. Factory setting: [01234567890123456789abcdef]
| [DHCP] | Sets whether to use automatic acquisition via DHCP when [INFRA] is selected in [TYPE]. [ENABLE]: Uses automatic acquisition. [DISABLE]: Does not use automatic acquisition. Set [IP ADDRESS], [SUBNET MASK], [DEFAULT GATEWAY], [PRIMARY DNS], and [SECONDARY DNS]. Factory setting: [ENABLE]
| [IP ADDRESS] | Sets the IP address when [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.1]
| [SUBNET MASK] | Sets the subnet mask when [DISABLE] is selected in [DHCP]. Factory setting: [255.255.255.0]
| [DEFAULT GATEWAY] | Sets the default gateway when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP]. Factory setting: [192.168.0.254]
| [PRIMARY DNS] | Sets the primary DNS server when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP], or when [ENABLE] is selected in [DHCP] and the primary DNS server cannot be obtained. Factory setting: [0.0.0.0]
| [SECONDARY DNS] | Sets the secondary DNS server when [INFRA] is selected in [TYPE] and [DISABLE] is selected in [DHCP], or when [ENABLE] is selected in [DHCP] and the primary DNS server cannot be obtained. Factory setting: [0.0.0.0]
| [DHCP SERVER] | Sets if the DHCP SERVER function is to be used or not when [DIRECT] is selected in [TYPE]. [ENABLE]: Uses the DHCP SERVER function. [DISABLE]: Does not use the DHCP SERVER function. Factory setting: [ENABLE]
[NETWORK TOOLS] | [STATUS DISPLAY] | Displays the network status.
| [INITIALIZE] | Restores the network setting status to the factory settings.

Top of the page