- Top
- Audio recording
- Preparing for audio input
- Using audio devices

# Using audio devices

1. <AUDIO IN 1> terminal

2. <AUDIO IN 2> terminal

3. <LINE>/<MIC> switch

Connect the audio device to the <AUDIO IN 1> or <AUDIO IN 2> terminal of the recording module using the XLR cable.

According to the channel to which the XLR cable is connected, select [REAR] in control panel audio input.

Switch the <LINE>/<MIC> switch on the <AUDIO IN 1> terminal or <AUDIO IN 2> terminal to <LINE>.

## Setting the control panel

Press the <HOME> button to display the HOME screen.

From [SYSTEM] → [AUDIO], select [AUDIO IN].

Select [REAR] in [CH1/2 IN].

[CH3/4 IN] is automatically set to [FRONT].

NOTE

- When the input signal is digital audio (AES/EBU format), set [MENU] → [SYSTEM SETTINGS] → [AUDIO INPUT] → [AES/EBU IN] to [ON]. All 4 channels become digital inputs, and audio input setting and level adjustment are disabled.

Top of the page