- Top
- Video Recording and Color Grading
- In-camera grading
- Control combinations through settings

# Control combinations through settings

[MAIN COLOR] | [Grading SEL] | [SUB COLOR] | [3D LUT] | [CDL] | Output Picture Adjustment
--- | --- | --- | --- | --- | ---
[MON 1] [MON 2] | [EVF] | [VF SDI]
[V-Log] | [External App]/[Internal] | [V-Log] | [OFF]/[V-709]/[Loaded File] | [ON]/[OFF] | V-Log Grading | V-Log Grading V-709 LCC | Same As VF/V-Log
[Grading]
[OFF] | [V-Log] | [OFF] | [OFF] | V-Log V-709 | V-Log V-709 LCC
[V-709]
[V-709] | [OFF] | [V-709] | [OFF] | [OFF] | V-709 | V-709 | Same As VF
[3D LUT] | [OFF] | [3D LUT] | [OFF] | [OFF] | 3D LUT | 3D LUT

When [MAIN COLOR] is set to [V-Log] or [3D LUT], the setting in [MENU] → [CAMERA SETTINGS] → [Enhanced] → [Enhanced SW] is fixed to [OFF].

When [Grading SEL] is set to [External App], the function is controlled from the color grading application of the computer connected via network. When [Grading SEL] is set to [Internal], the function is controlled from the control panel.

Color grading operations can be performed using CDL even while recording is in operation. The CDL parameter value to record as the .cdl file becomes the value when recording stops.

The control parameter recorded in the file and the control parameter applied to the video may not match when an operation for color grading is performed right before stopping the recording.

Picture adjustment matching the settings of the output picture adjustment is output when playing the recorded V-Log video.

The .vlt and CDL parameters that is currently set in the camera is applied rather than the .vlt or .cdl that is saved at the same time as the clip to play when set to Grading.

#### When playing back the recorded V-Log video

When outputting in output picture adjustment

- Select [OFF] in [MENU] → [SYSTEM SETTINGS] → [COLOR SETTING] → [PLAYBACK GRADING].

- This is reflected to the output with [MON 1]/[MON 2]/[VF]/[VF SDI] setting is set to [Grading].

When outputting with the control parameter recorded in the P2 card

- Select [ON] in [MENU] → [SYSTEM SETTINGS] → [COLOR SETTING] → [PLAYBACK GRADING].

- This is reflected to all output regardless of [MON 1]/[MON 2]/[VF]/[VF SDI] setting.

NOTE

- When playing back V-RAW recorder with VariCam 35

  The picture adjustment by the control parameter is not performed even when [PLAYBACK GRADING] is set to [ON].

- The V-Log video with the [3D LUT] file other than the [V-709] setting recorded by VariCam 35 attached

  VariCam HS will not perform the picture adjustment by the saved control parameter even when [PLAYBACK GRADING] is set to [ON].

Top of the page