- Top
- Network Connection
- Connecting the remote operation panel (AK-HRP200G)
- Limitation with the remote control

# Limitation with the remote control

There are following limitations when controlling from the remote operation panel.

#### When the [MENU] → [CAMERA SETTINGS] → [Enhanced] → [Enhanced SW] is set to [ON]

- Camera power button <HEAD POWER>: Control is not possible

- Automatic white balance button <WHITE>: Aborting during adjustment is not possible

- Automatic black balance button <BLACK>: Aborting during adjustment is not possible

- Automatic setup button <SETUP>: Not used

- 5600 K button <5600 K>: Not used

- Knee off button <KNEE OFF>: Disabled

- Scene/user file switching button <SHIFT>: Disabled

- Scene/user file selection buttons <SCENE1/USER1> - <SCENE3/USER3>/<SCENE4>: Disabled

- Scene/user file registration button<STORE>: Disabled

- Volume lock button <VR LOCK>: Enabled

- R flare/pedestal volume <FLARE/PED R>: Disabled

- B flare/pedestal volume <FLARE/PED B>: Disabled

- Dataset buttons <UP>/<DOWN>: Enabled

- Adjusted value display area (4 digits): Enabled

- Camera number display area <No.>: Enabled

- Camera selection button <SELECT>: Enabled

- Memory card slot: Disabled

- Red/green tally display area, call button <TALLY/CALL>: Disabled

- Iris/master pedestal lock button <IRIS/M.PED LOCK>: Enabled

- Iris lever <IRIS>: Enabled when the lens can operate

- Sense volume <SENSE>: Disabled

- Coarse volume <COARSE>: Disabled

- Auto iris button <AUTO>: Enabled when the lens can operate

- Iris close button <CLOSE>: Enabled when the lens can operate

- Fader full button <FULL>: Disabled

- Alarm display area <ALM>: Warning is displayed

- Light alarm display area <OPT>: Disabled

- Lens extender display <EXT>: Enabled when the lens can operate

- Digital extender display <D.EXT>: Disabled

#### When the [MENU] → [CAMERA SETTINGS] → [Enhanced] → [Enhanced SW] is set to [OFF]

Following buttons are disabled in addition to limitation when [Enhanced SW] is set to [ON].

- Matrix button <MATRIX>

- Skin tone detail button <SKINDTL>

- Detail off button <DTL OFF>

- Detail volume <DTL>

- RGain volume <GAIN R>

- BGain volume <GAIN B>

- RFlare/pedestal volume <FLARE/PED R>

- BFlare/pedestal volume <FLARE/PED B>

- Master pedestal volume <M.PED>

## About adjusted value display area (4 digits)

Zoom, focus, and auto focus are not supported.

When the VFR is set to [ON], it is displayed as [P] ( is the frame rate value).

When the VFR is set to [OFF], it is displayed as [FroF].

When the setting of the camera is set to [Native ISO] or [ISO], it is displayed as [iSo].

NOTE

- To connect the camera and AK-HRP200G directly, use a crossover LAN cable.

- For details, refer to the Operating Instructions of AK-HRP200G.

- The following information is required to connect to AK-HRP200G.

  - User account name

  - Password

  - IP address

  - Port number: 49152

- For AK-HRP200G, use Ver.4.01.00 or later versions.

- For details on the operations of ROP setup software application, refer to the Operating Instructions of AK-HRP200G.

- For the ROP setup software application, use Ver.3.0.0.0 or later versions.

Top of the page