- Top
- Menu Operations
- Menu list
- [CAMERA SETTINGS]

# [CAMERA SETTINGS]

Sets the fine quality adjustment of camera videos and camera operation.

is the extended menu. Set [MENU] → [CAMERA SETTINGS] → [Enhanced] → [Enhanced SW] to [ON] to display the extended menu.

Item | Description of settings
--- | ---
[Enhanced] | [Enhanced SW] | Enables/disables the [Enhanced] function. [ON]: Enables the [Enhanced] function and shows the menu related to the [Enhanced] function. [OFF]: Disables the [Enhanced] function and hides the menu related to the [Enhanced] function. Factory setting: [OFF]
[FPS] | [VFR SW] | Enables/disables the variable frame rate function. [ON]: Enables the variable frame rate function. The desired frame rate can be set using [PRESET VALUE]/[VARIABLE VALUE]. Audio cannot be recorded. [OFF]: Disables the variable frame rate function. [VFR SW] is fixed to [ON] when [SYSTEM SETTINGS] → [SYSTEM MODE] → [HIGH SPEED] is set to [ON (1-fps)]. Factory setting: [OFF]
| [FPS MODE] | Selects the frame rate setting method. [PRESET]: Selects the frame rate from preset frame rates (maximum of 12). Registration is done from the control panel. [VARIABLE]: Selects the frame rate from all available frame rates. Factory setting: [PRESET]
| [PRESET VALUE] | Selects a value from a maximum of 12 values set from the control panel. Factory setting: [24fps]
| [VARIABLE VALUE] | Selects the frame rate from all available frame rates. Selectable values vary depending on [SYSTEM MODE] settings. Factory setting: [24fps]
[WHITE] | [AWB] | Executes automatic white balancing. [EXECUTE], [CANCEL] Factory setting: [CANCEL]
| [MODE] | Selects the white balance mode. [PRESET]: Selects the color temperature from preset color temperatures. Registration is done from the control panel. [TEMP SHIFT]: Selects the color temperature from all configurable color temperatures. Factory setting: [PRESET]
| [PRESET VALUE] | Selects a value from a maximum of 12 values set from the control panel. Preset values that can be selected in the factory setting are [3200K+0GMg], [4300K+0GMg], [5600(5500)K+0GMg], and [6300K+0GMg]. Factory setting: [3200K+0GMg]
| [TEMP SHIFT] | Selects the color temperature from all configurable color temperatures. [2300K]…[15000K] Factory setting: [3200K]
| [GMg] | Adjusts the balance between green and magenta. +: Adjusts toward green. −: Adjusts toward magenta. [−10]…[10] Factory setting: [0]
| [R GAIN] | Adjusts the Rch gain. [−200]…[200] Factory setting: [0]
| [B GAIN] | Adjusts the Bch gain. [−200]…[200] Factory setting: [0]
| [AWB OFFSET] | Sets the Rch gain and Bch gain value when performing automatic white balancing. [ON]: Maintains and adds the values of [R GAIN] and [B GAIN] after performing automatic white balancing. [OFF]: Resets the value of [R GAIN] and [B GAIN] after performing automatic white balancing. Factory setting: [OFF]
| [SHOCKLESS WHITE] | Sets the transition time when switching preset values. [OFF]: Values are immediately switched. [1]: Switches in approximately one second. [2]: Switches in approximately two seconds. [3]: Switches in approximately five seconds. Factory setting: [OFF]
[BLACK] | [ABB] | Executes automatic black balancing. When executing automatic black balancing, put the cap on the lens to keep any light from entering the image sensor. [EXECUTE], [CANCEL] Factory setting: [CANCEL]
| [M.PED] | Sets the master pedestal level. [−100]…[100] Factory setting: [0]
| [R PED] | Adjusts the Rch pedestal level. [−100]…[100] Factory setting: [0]
| [G PED] | Adjusts the Gch pedestal level. [−100]…[100] Factory setting: [0]
| [B PED] | Adjusts the Bch pedestal level. [−100]…[100] Factory setting: [0]
| [ABB OFFSET] | Sets the pedestal levels for Rch, Gch, and Bch after performing the adjustment of the automatic black balance. [ON]: The values of [R PED], [G PED], and [B PED] are maintained and added even after performing the automatic black balance. [OFF]: The values of [R PED], [G PED], and [B PED] are reset after performing the automatic black balance. Factory setting: [OFF]
| [INITIAL ABB] | Executes the initialization of the sensor at the same time the automatic black balance is executed. This can be selected only when [HIGH SPEED] is set to [ON]. Keep the light away from the image sensor by placing a cap on the lens, etc., when executing the automatic black balance. [EXECUTE], [CANCEL] Factory setting: [CANCEL]
[NR] | [ISO800] | Switches the noise reduction effect in the range of ISO200 to ISO4000. [ON], [OFF] The range will be ISO200 to ISO2000 when [HIGH SPEED] is set to [ON]. The range will be 0 dB to 15 dB when [MODE] in [EI] is set to [dB]. Factory setting: [OFF]
| [ISO5000] | Switches the noise reduction effect in the range of ISO5000 to ISO12800. [ON], [OFF] The range will be ISO2500 to ISO6400 when [HIGH SPEED] is set to [ON]. The range will be 18 dB to 24 dB when [MODE] in [EI] is set to [dB]. Factory setting: [OFF]
[EI] | [MODE] | Switches the EXPOSURE INDEX control unit. [ISO], [dB] Factory setting: [ISO]
| [ISO SELECT] | Selects the operation of ISO. [NATIVE ONLY], [800BASE], [5000BASE] Factory setting: [NATIVE ONLY]
| [NATIVE ISO] | Sets the value when [NATIVE ONLY] is selected. [800], [5000] The value will be [400] and [2500] when [HIGH SPEED] is set to [ON]. Factory setting: [800]
| [800BASE ISO] | Sets the value when [800BASE] is selected. [200], [250], [320], [400], [500], [640], [800], [1000], [1250], [1600], [2000], [2500], [3200], [4000], [5000], [6400], [8000], [10000], [12800] It will be [200], [250], [320], [400], [500], [640], [800], [1000], [1250], [1600], [2000], [2500], [3200], [4000], [5000], and [6400] when the setting of [HIGH SPEED] is [ON]. Factory setting: [800]
| [5000BASE ISO] | Sets the value when [5000BASE] is selected. [1250], [1600], [2000], [2500], [3200], [4000], [5000], [6400], [8000], [10000], [12800] It will be [1250], [1600], [2000], [2500], [3200], [4000], [5000], and [6400] when [HIGH SPEED] is set to [ON]. Factory setting: [5000]
| [SETTING(GAIN)] | Sets the value when [dB] is selected. [0dB], [3dB], [6dB], [9dB], [12dB], [15dB], [18dB], [21dB], [24dB] Factory setting: [0dB]
| [GAIN OFFSET SW] | Sets whether to perform fine adjustment of control when [dB] is selected. [ON], [OFF] Factory setting: [OFF]
| [OFFSET LEVEL] | Sets the fine adjustment level. [0.0dB] - [0.9dB] (0.1 dB step) Factory setting: [0dB]
[SHUTTER] | [SW] | Enables/disables the shutter function. [ON], [OFF] Factory setting: [ON]
| [DISPLAY MODE] | Sets the shutter display unit. [sec]: Displays in time. [deg]: Displays at shutter open angle. Factory setting: [deg]
| [MODE] | Switches the shutter control mode. [PRESET]: Selects the mode from 12 modes inside the memory. [SYNCHRO]: Selects the mode from the operable range. Factory setting: [PRESET]
| [SYNCHRO deg] | Sets the value of angle control ([deg]). [1.0]…[358.0] Factory setting: [180.0]
| [SYNCHRO sec] | Sets the value of time control ([sec]). The lowest value changes depending on the frame rate ([FPS]) value. [1/60] - [1/250] Factory setting: [1/48]
| [PRESET VALUE deg] | Selects the angle control ([deg]) value from the maximum of 12 values set in the control panel. Preset values that can be selected in the factory setting are [11.5], [22.5], [45.0], [90.0], [120.0], [144.0], [172.8], [180.0], [270.0], and [358.0]. Factory setting: [180.0]
| [PRESET VALUE sec] | Selects the time control ([sec]) value from the maximum of 12 values set in the control panel. Preset values that can be selected in the factory setting are [1/60], [1/100], [1/120], [1/250], [1/500], [1/1000], and [1/2000]. Factory setting: [1/60]
[TEST SIG] | [TEST SIG SEL] | Sets the test signal output. [OFF]: Does not output a test signal. [BARS]: Outputs the color bar set in [COLOR BARS TYPE]. Factory setting: [OFF]
| [COLOR BARS TYPE] | Set the color bar to be used. [SMPTE]: Uses the color bar in the SMPTE standard. [FULL]: Uses full color bars. Factory setting: [SMPTE]
[DETAIL] | [SW] | Enables/disables the detail function. [ON], [OFF] Factory setting: [OFF]
| [CORING] | Sets the coring amount for the detail signal. [0] - [60] Factory setting: [1]
| [MASTER LEVEL] | Sets the effect level for the detail signal. [−31]…[31] Factory setting: [0]
[SKIN DETAIL] | [SW] | Enables/disables the skin tone detail function. [OFF], [ON] Factory setting: [OFF]
| [TABLE SELECT] | Selects the table for the skin tone detail. [A], [B], [C], [A+B], [A+C], [B+C], [A+B+C] Factory setting: [A]
| [GET] | Sets whether to register the screen center color as the color by which the skin tone detail is applied. [EXECUTE], [CANCEL]
| [ZEBRA SW] | Sets whether to superimpose the zebra signal to the color by which the skin tone detail is applied. [ON], [OFF] Factory setting: [OFF]
| [EFFECT LEVEL] | Sets the effective level of the skin tone detail. The higher the value, the more significant the effect. [0] - [31] Factory setting: [16]
| [DETECT TABLE] | Selects the skin tone table of the subject that displays the skin tone detail. [A], [B], [C] Factory setting: [A]
| [I CENTER] | Sets the center position of the upper I axis (setting the area that displays the skin tone). [0]…[255] Factory setting: [35]
| [I WIDTH] | Sets the width of the area that displays the skin tone of the upper I axis that focus on [I CENTER]. [0]…[255] Factory setting: [55]
| [Q WIDTH] | Sets the width of the area that displays the skin tone of the upper Q axis that focus on [I CENTER]. [0]…[127] Factory setting: [22]
| [Q PHASE] | Sets the phase of the area that displays the skin tone regarding to the Q axis. [0]…[255] Factory setting: [0]
[MATRIX] | [SW] | Enables/disables the matrix function. [ON], [OFF] Factory setting: [OFF]
| [(R-G)_N] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(R-G)_P] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(R-B)_N] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(R-B)_P] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(G-R)_N] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(G-R)_P] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(G-B)_N] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(G-B)_P] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(B-R)_N] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(B-R)_P] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(B-G)_N] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
| [(B-G)_P] | Adjusts the linear matrix. [−127]…[127] Factory setting: [0]
[COLOR CORRECTION] | [SW] | Enables/disables the color correction function. [ON], [OFF] Factory setting: [OFF]
| [R (SAT)] | Corrects red color saturation. [−63]…[63] Factory setting: [0]
| [R (PHASE)] | Corrects the red hue. [−63]…[63] Factory setting: [0]
| [R-Mg (SAT)] | Corrects the color saturation between red and magenta. [−63]…[63] Factory setting: [0]
| [R-Mg (PHASE)] | Corrects the hue between red and magenta. [−63]…[63] Factory setting: [0]
| [Mg (SAT)] | Corrects magenta color saturation. [−63]…[63] Factory setting: [0]
| [Mg (PHASE)] | Corrects the magenta hue. [−63]…[63] Factory setting: [0]
| [Mg-B (SAT)] | Corrects the color saturation between magenta and blue. [−63]…[63] Factory setting: [0]
| [Mg-B (PHASE)] | Corrects the hue between magenta and blue. [−63]…[63] Factory setting: [0]
| [B (SAT)] | Corrects blue color saturation. [−63]…[63] Factory setting: [0]
| [B (PHASE)] | Corrects the blue hue. [−63]…[63] Factory setting: [0]
| [B-Cy (SAT)] | Corrects the color saturation between blue and cyan. [−63]…[63] Factory setting: [0]
| [B-Cy (PHASE)] | Corrects the hue between blue and cyan. [−63]…[63] Factory setting: [0]
| [Cy (SAT)] | Corrects cyan color saturation. [−63]…[63] Factory setting: [0]
| [Cy (PHASE)] | Corrects the cyan hue. [−63]…[63] Factory setting: [0]
| [Cy-G (SAT)] | Corrects the color saturation between cyan and green. [−63]…[63] Factory setting: [0]
| [Cy-G (PHASE)] | Corrects the hue between cyan and green. [−63]…[63] Factory setting: [0]
| [G (SAT)] | Corrects green color saturation. [−63]…[63] Factory setting: [0]
| [G (PHASE)] | Corrects the green hue. [−63]…[63] Factory setting: [0]
| [G-Yl (SAT)] | Corrects the color saturation between green and yellow. [−63]…[63] Factory setting: [0]
| [G-Yl (PHASE)] | Corrects the hue between green and yellow. [−63]…[63] Factory setting: [0]
| [Yl (SAT)] | Corrects yellow color saturation. [−63]…[63] Factory setting: [0]
| [Yl (PHASE)] | Corrects the yellow hue. [−63]…[63] Factory setting: [0]
| [Yl-R (SAT)] | Corrects the color saturation between yellow and red. [−63]…[63] Factory setting: [0]
| [Yl-R (PHASE)] | Corrects the hue between yellow and red. [−63]…[63] Factory setting: [0]
[SKIN CORRECTION] | [SKIN AREA SW] | Enables/disables the function which makes fine adjustments of near skin tone colors. [ON], [OFF] Factory setting: [OFF]
| [SKIN AREA HUE] | Makes fine adjustments in hue. [−63]…[63] Factory setting: [0]
| [SKIN AREA TONE] | Makes fine adjustments in tone. [−63]…[63] Factory setting: [0]
[EXT.FUNC] | [FOCUS DISP] | Sets the unit that displays the focus distance. [Meter], [Feet] Factory setting: [Feet]
[LENS SETTING] | [A.IRIS TYPE] | Determines whether to set the speed control to the lens volume and use the value set in the menu. [LENS], [CAM] Factory setting: [LENS]
| [A.IRIS LEVEL EFFECT] | Sets the target value during auto iris operation. [0] - [100] Factory setting: [30]
| [A.IRIS SPEED] | Sets the speed when the [A.IRIS TYPE] is set to [CAM]. [1] - [20] Factory setting: [10]
| [A.IRIS WINDOW] | Selects the auto iris detection window. [NORMAL1]: Window that is near screen center. [NORMAL2]: Window that is near screen bottom. [CENTER]: Window that is a spot in the screen center. Factory setting: [NORMAL1]
| [A.IRIS PEAK/AVE] | Sets the ratio included in the peak for auto iris standard. [0] - [100] Factory setting: [30]
| [LENS CONNECT TYPE] | Sets the type of lens to be connected. [TYPE A]: Lens controlled with LDS (Lens Data System). (ULTRA PRIME lens not supported) [TYPE B]: Lens controlled with 12-pin connector [TYPE C]: Lens controlled with cooke/i communication [OFF]: Other lenses Factory setting: [OFF]

Top of the page