- Top
- Audio recording
- Selecting audio input and adjusting recording levels
- Selecting audio input signals

# Selecting audio input signals

Press the <HOME> button to display the HOME screen.

From [SYSTEM] → [AUDIO], select [AUDIO IN].

Select [FRONT] in [CH1/2 IN].

[CH3/4 IN] is automatically set to [REAR].

NOTE

- When the input signal is in AES/EBU format, all 4 channels become AES/EBU input, and audio input signal setting is disabled.

- The audio signal to be recorded is output straight as SDI signal. The details regarding audio is set in [MENU] → [SYSTEM SETTINGS] → [AUDIO INPUT], [AUDIO LEVEL], and [AUDIO OUTPUT].

Top of the page