- Top
- Control Panel
- HOME screen

# HOME screen

The Home screen displays the basic camera settings and is used to change those settings.

[FPS] | Sets the frame rate.
[VFR] | Toggles the variable frame rate. When this is [OFF], the frame rate become 1x the rate set in [MENU] → [SYSTEM SETTING] → [FREQUENCY]. When this is [ON], audio cannot be recorded. Audio is recorded at the sub recorder.
[PRESET] | Mode for selecting preset frame rates. Up to 12 presets can be stored in memory. Presets can be added/deleted using [ADD]/[DEL].
[VARIABLE] | Mode for selecting from the overall variable range. The variable step changes through [FINE]/[NORMAL]/[COARSE].
[SHUTTER] | Sets the shutter speed.
[ON]/[OFF] | [OFF] means shutter off (open angle 360 deg).
[PRESET] | Mode for selecting preset shutter speeds. Up to 12 can be registered. Presets can be added/deleted using [ADD]/[DEL].
[SYNCHRO] | Mode for selecting from the overall variable range. The variable step changes through [FINE]/[COARSE].
[deg/sec] | Determines the shutter setting unit. [deg]: Open angle [sec]: Second
[EI] | Sets the EXPOSURE INDEX (gain).
[ISO/dB] | Selects the setting method.
[NATIVE ONLY] | Only the native ISO can be selected. (when [ISO] is set)
[800BASE] | The ISO800 standard value can be selected. (when [ISO] is set)
[5000BASE] | The ISO5000 standard value can be selected. (when [ISO] is set)
[WB] | Sets the color temperature (white balance).
[AWB] | Executes automatic white balancing.
[PRESET] | Mode for selecting preset white balance values. Up to 12 can be registered. Presets can be added/deleted using [ADD]/[DEL]. If [AWB] is performed, the results are automatically added to the choices.
[TEMP SHIFT] | Mode for making adjustments from the overall variable range.
[GMg] | Shifts to the Green-Magenta axis.
[COLOR] | Sets the video colors (gamma and gamut).
| [MAIN COLOR] | Sets the output colors of videos from terminals <SDI OUT1> to <SDI OUT4> as well as videos recorded in the main recorder.
| [SUB COLOR] | Sets the colors of videos recorded in the sub recorder.
| [Grading SEL] | Sets the grading function. [MAIN COLOR] is only enabled in [V-Log] mode.
| [3D LUT] | Sets the grading in the [3D LUT]. [Grading SEL] is disabled when this is [OFF]. When [Grading SEL] is set to [Internal] or [External App] Loads from the SD memory card using [LOAD]. Saves the setting value to the SD memory card with [SAVE AS].
| [CDL] | Sets the grading in [CDL]. [Grading SEL] is disabled when this is [OFF]. When [Grading SEL] is set to [Internal] or [External App] Sets [Slope]/[Offset]/[Power]/[Saturation] on the control panel. Loads from the SD memory card using [LOAD]. Saves the setting value to the SD memory card with [SAVE AS].
| [MON SET] | Sets the display color for [MON OUT]/[VF]/[VF SDI].
[SYSTEM MODE] | Sets the camera’s system.
[FREQUENCY] | Sets the system frequency.
[PIXEL] | Sets the camera’s main resolution (number of pixels).
[MAIN CODEC] | Sets the main recorder’s codec. The camera’s basic system is determined by four settings: [FREQUENCY], [PIXEL], [MAIN CODEC], and [HIGH SPEED]. Restarting the system may be necessary if basic system settings are changed. After confirming the four settings, restart in accordance with the guide.
[SUB CODEC] | [SUB CODEC]: Sets the codec of the sub recorder. [VFR SUB REC]: Selects either [NORMAL+Audio] or [VFR up to 60p (50p)]. [NORMAL+Audio]: Records in the frame of system frequency. Audio signal is also recorded. [VFR up to 60p (50p)]: Records in a variable frame rate by synchronizing to the [VFR] setting of the main recorder. Audio signal is not recorded when [VFR] is set to [ON]. Recording is not available when the frame rate is 60p (50p) display or higher.
[HIGH SPEED] | Sets the high speed mode. Playback operation is not possible when [MAIN CODEC] is set to ProRes format and [HIGH SPEED] is set to [ON].
[AUDIO] | [AUDIO] | Sets the audio input and recording. [VOL]: Sets the input volume. [IN]: Sets input channel switching and level control. [OUT]: Sets the output to a speaker or headphone.
[DAILIES] | Sets the data to superimpose on the video to be recorded in the sub recorder.
[WATER MARK] | Superimposes the set character string.
[FRAME MARK] | Superimposes the frame mark.
[WINDOW BURN] | Sets [WINDOW BURN].
[BURN DATA] | Sets [BURN DATA] used in [WINDOW BURN].
[PREVIEW] | Checks the setting status of [WINDOW BURN].
[USER CLIP NAME] | Sets [USER CLIP NAME].
[CAM INDEX] | Sets the [CAM INDEX] applicable when the [USER CLIP NAME] is set to [TYPE3].
[NEXT REEL COUNT] | Sets the [NEXT REEL COUNT] applicable when the [USER CLIP NAME] is set to [TYPE3].
[TYPE] | Sets [TYPE] of [USER CLIP NAME].

Top of the page