- Top
- Extension module
- Connecting to the DC output terminal
- Connecting to the <DC OUT> terminal

# Connecting to the <DC OUT> terminal

It is possible to get a 1.0 A current from the <DC OUT> terminal of the camera extension module.

Cable connector

0B.302

LEMO

1. GND

2. +12 V

NOTE

- Make sure that polarity is correct before connecting an external device. Otherwise, it may result in a malfunction.

Top of the page