- Top
- Video Recording and Color Grading
- Special recording functions
- Hot swap recording

# Hot swap recording

When P2 cards are inserted into two card slots, recording can be performed continuously across two cards.

Also, the card other than the one currently being recorded to can be swapped and recording can be continued on three or more cards (hot swap recording).

However, P2 card recognition might slow down depending on the timing (before and after continuous recording across two card slots) that the P2 card is inserted into the vacant card slot. When inserting a P2 card, make sure that there is at least one minute of free space on the card to be recorded to.

NOTE

- Hot swap playback is not supported.

- The hot swap recording is not possible with the ProRes format.

- The hot swap recording cannot be performed when [CINE] is selected for file name style.

Top of the page