- Top
- Menu Operations
- Menu list
- [AUDIO SETTINGS]

# [AUDIO SETTINGS]

Various setting items for audio recording.

Item | Description of settings
--- | ---
[AUDIO RECORD] | Sets whether to record the audio. The audio data itself is not recorded when set to [OFF]. (Audio data will not appear in the timeline of editing software) [ON], [OFF] Factory setting: [ON]
[AUDIO INPUT] | [AES/EBU IN] | If this is set to [ON], the digital audio (AES/EBU standard-compliant) input from the <AUDIO IN 1> terminal and <AUDIO IN 2> terminal is recorded in 4 channels. In this case, analog input selection and volume adjustment is not possible. [ON], [OFF] Factory setting: [OFF]
| [FRONT MIC POWER] | Enables/disables the front microphone phantom power. [ON], [OFF] Factory setting: [ON]
| [FRONT MIC LEVEL] | Sets the front microphone input level. [−40dB], [−50dB] Factory setting: [−40dB]
| [REAR1 MIC POWER] | Enables/disables the phantom power of the rear microphone connected to the <AUDIO IN 1> terminal. [ON], [OFF] Factory setting: [OFF]
| [REAR2 MIC POWER] | Enables/disables the phantom power of the rear microphone connected to the <AUDIO IN 2> terminal. [ON], [OFF] Factory setting: [OFF]
| [REAR MIC LEVEL] | Sets the input level of the rear microphone connected to the <AUDIO IN 1> and <AUDIO IN 2> terminals. [−40dB], [−50dB], [−60dB] Factory setting: [−60dB]
| [REAR LINE LEVEL] | Sets the line input level from the <AUDIO IN 1> terminal and <AUDIO IN 2> terminal. [4dB], [0dB], [−3dB] Factory setting: [4dB]
| [FRONT1 MIC LOWCUT] | Enables/disables the low-cut filter of front microphone 1. [ON], [OFF] Factory setting: [OFF]
| [FRONT2 MIC LOWCUT] | Enables/disables the low-cut filter of front microphone 2. [ON], [OFF] Factory setting: [OFF]
| [REAR1 MIC LOWCUT] | Enables/disables the low-cut filter of rear microphone 1. [ON], [OFF] Factory setting: [OFF]
| [REAR2 MIC LOWCUT] | Enables/disables the low-cut filter of rear microphone 2. [ON], [OFF] Factory setting: [OFF]
| [CH IN SEL] | Sets the input of audio channels 1 to 4. [1･2FRONT 3･4REAR], [1･2REAR 3･4FRONT] Factory setting: [1･2FRONT 3･4REAR]
| [TEST TONE] | Sets whether to output a test signal when the video is made to a color bar. [ON]: Outputs a test tone. [OFF]: Does not output a test tone. Factory setting: [ON]
[AUDIO LEVEL] | [FRONT1 LEVEL] | Sets the level adjustment method of the front microphone 1 to manual or automatic. [AUTO]: Adjust automatically. [MANUAL]: Enables manual adjustment. Factory setting: [AUTO]
| [FRONT2 LEVEL] | Sets the level adjustment method of the front microphone 2 to manual or automatic. [AUTO]: Adjust automatically. [MANUAL]: Enables manual adjustment. Factory setting: [AUTO]
| [REAR1 LEVEL] | Sets the level adjustment method of the rear microphone 1 to manual or automatic. [AUTO]: Adjust automatically. [MANUAL]: Enables manual adjustment. Factory setting: [AUTO]
| [REAR2 LEVEL] | Sets the level adjustment method of the rear microphone 2 to manual or automatic. [AUTO]: Adjust automatically. [MANUAL]: Enables manual adjustment. Factory setting: [AUTO]
| [FRONT1 VOL] | Performs adjustments in this item when the level adjustment method of the front microphone 1 is set to [MANUAL]. [0]…[100] Factory setting: [70]
| [FRONT2 VOL] | Performs adjustments in this item when the level adjustment method of the front microphone 2 is set to [MANUAL]. [0]…[100] Factory setting: [70]
| [REAR1 VOL] | Performs adjustments in this item when the level adjustment method of the rear microphone 1 is set to [MANUAL]. [0]…[100] Factory setting: [70]
| [REAR2 VOL] | Performs adjustments in this item when the level adjustment method of the rear microphone 2 is set to [MANUAL]. [0]…[100] Factory setting: [70]
| [FRONT1 LIMITER] | Enables/disables the limiter of front microphone 1. [ON], [OFF] Factory setting: [OFF]
| [FRONT2 LIMITER] | Enables/disables the limiter of front microphone 2. [ON], [OFF] Factory setting: [OFF]
| [REAR1 LIMITER] | Enables/disables the limiter of rear microphone 1. [ON], [OFF] Factory setting: [OFF]
| [REAR2 LIMITER] | Enables/disables the limiter of rear microphone 2. [ON], [OFF] Factory setting: [OFF]
| [HEADROOM] | Sets the headroom (standard level). [18dB], [20dB] Factory setting: [20dB]
[AUDIO OUTPUT] | [MONITOR SEL1] | Sets the audio channel to be output from the <PHONES> terminal. [CH1/2]: Outputs audio channel 1/2. [CH3/4]: Outputs audio channel 3/4. Factory setting: [CH1/2]
| [MONITOR SEL2] | Sets the audio format (mono, stereo, mix) to be output from the <PHONES> terminal. When [MONITOR SEL1] is set to [CH1/2]: [MONO CH1], [MONO CH2], [STEREO CH1/2], [MIX CH1/2] When [MONITOR SEL1] is set to [CH3/4]: [MONO CH3], [MONO CH4], [STEREO CH3/4], [MIX CH3/4] Factory setting: [STEREO CH1/2] or [STEREO CH3/4]
| [MONITOR DELAY] | Sets whether to delay the audio from the <PHONES> terminal to match the monitor output. [ON], [OFF] Factory setting: [OFF]
| [MONITOR VOL] | Adjusts the level of audio to be output from the <PHONES> terminal. [0]…[100] Factory setting: [70]
| [ALARM] | Sets the volume of the warning sound to be output from the <PHONES> terminal. [LOUD], [MEDIUM], [SMALL], [OFF] Factory setting: [MEDIUM]

Top of the page