- Top
- V-RAW recorder
- V-RAW recorder
- Attaching the V-RAW recorder

# Attaching the V-RAW recorder

V-RAW recorder is attached to the battery holder and the external unit connection terminal of the recording module.

Cover

Fig. 1

Fig. 2

Fig. 3

Fig. 4

Loosen the screw on the external unit connection terminal at the rear of the recording module and remove the cover. (Fig. 1)

Attach the V-RAW recorder. (Fig. 2)

Slide the V-RAW recorder downward. (Fig. 3)

Fold down the release lever of the V-RAW recorder. (Fig. 4)

## Disassembling

Stopper

Fig. 1

Fig. 2

Fig. 3

Slide the stopper on the release lever on the V-RAW recorder, and pull up the release lever. (Fig. 1, Fig. 2)

The V-RAW recorder will lift.

Remove the V-RAW recorder. (Fig. 3)

Top of the page