- Top
- Network Connection
- Preparing for connection
- For wireless LAN

# For wireless LAN

Attach the wireless module AJ-WM30/AJ-WM50 (optional) to the camera.

Fig. 1

Fig. 2

Fig. 3

Push the lever down, and open the cover. (Fig. 1, Fig. 2)

Connect the wireless module to the <USB HOST> terminal. (Fig. 3)

Insert it all the way.

Close the cover.

NOTE

- When removing the wireless module, pull it down straight.

- When connected with the wireless LAN, attach the wireless module securely and close the cover.

## Cautions when using wireless module AJ-WM30/AJ-WM50

Read the operating manual of the wireless module thoroughly and understand it before using.

For the latest information, visit the following website:

https://pro-av.panasonic.net/

Top of the page