- Top
- Description of Parts
- Camera module
- Right side

# Right side

1. Accessory mounting holes

   For attaching accessories.

   - Mounting hole size

     - 3/8-16 UNC

2. Fan outlet

   Fan outlet for dissipating heat. Do not block this when the camera is in use.

3. Recording module release lever

   Lever for removing the recording module (optional) from the camera module.

4. Accessory mounting holes

   For attaching accessories.

   - Mounting hole size

     - 1/4-20 UNC (screw length 5.5 mm or shorter)

5. USER button (<4>)

   User-selected functions can be assigned to this button. Pressing the button performs the assigned function.

6. Focus hook

   Indicate the focal plane of the MOS sensor. It provides a reference for measuring the accurate focal length from the subject.

7. <VF> terminal

   Terminal for connecting the HD viewfinder AU-VCVF1G (optional).

8. <VF SDI> terminal

   Output terminal for 3G/HD SDI. Displays the video equal to the viewfinder display.

   For the cable to connect to this terminal, prepare a double-shielded cable equivalent to 5C-FB.

9. <DC OUT> terminal

   This is the DC12 V output terminal. It provides a maximum current of 1 A.

10. <MIC IN> terminal

    Terminal for connecting a microphone.

11. <LENS> terminal

    Terminal for connecting a lens cable. For details, refer to the Operating Instructions for the lens.

Top of the page