- Top
- Video Recording and Color Grading
- P2 card
- Removing a P2 card

# Removing a P2 card

Fig. 1

Fig. 2

Open the card slot cover.

Remove the card.

- expressP2 memory cards

  - Slide the main slot lock switch to the left to release the lock.

  - Lift the eject button (Fig. 1), and press in. (Fig. 2)

- microP2 memory cards

  - Press in the microP2 card further into the camera and let go.

  - The microP2 memory card is released from the card slot, and the microP2 memory card can be removed.

NOTE

- Do not remove the P2 card after inserting it, while it is being accessed, or being detected (card access LED flashing in orange). Otherwise, it may result in a malfunction.

- If the P2 card is removed while being accessed, [TURN POWER OFF] is displayed on the viewfinder screen, and the camera gives out a warning indication by a warning lamp, etc. Also, all card access LEDs flash rapidly in orange. Turn off the power. (Warning system)

- If the P2 card is removed while being accessed, clips on it may become irregular. Check the clips and restore them, if required.

- If the P2 card being formatted is removed, formatting of the P2 card is not guaranteed. In this case, [TURN POWER OFF] is displayed on the viewfinder screen displays. Turn off the power and then back on again, and reformat the P2 card.

- If a P2 card is inserted into another slot during playback, the inserted card is not recognized and the card access LED does not light up. The P2 card will start to be recognized when playback ends.

- Even if a P2 card is inserted in a vacant card slot during recording, the P2 card may not be recognized immediately in the following instance:

  - Immediately after a recording slot is switched

Top of the page