- Top
- Extension module
- Description of parts
- Left side

# Left side

: Camera extension module

: Recording extension module

1. <DC OUT> terminal

   This is the DC12 V output terminal. The DC output provides a maximum current of 1.0 A.

2. <SIX USER BUTTONS> button

   This button sets the control panel operation buttons of the recording module (optional) to be used as USER buttons. You can operate the functions allocated from [USER5] to [USER10] in [MENU] → [SYSTEM SETTINGS] → [USER SWITCHES].

Top of the page