- Top
- V-RAW recorder
- Operation with the control panel
- System setting and recording

# System setting and recording

The camera main unit and the V-RAW recorder will operate as a single system. All the operations of the V-RAW recorder can be operated on the control panel of the recording module. The recording can also be started/stopped with the <REC> button on the recording module.

#### [SYSTEM] setting screen

#### [V-RAW] format setting screen

Priority of the setting is as follows.

1. [FREQUENCY]

2. [V-RAW]

3. [MAIN PIXEL]

4. [MAIN CODEC]

5. [SUB CODEC]

The setting value for lower order is also changed when the setting value of higher order is changed.

Example)

- When [FREQUENCY] is set to 30p or less, all [V-RAW] ([4K/12bit], [UHD/12bit], [4K/10bit], and [UHD/10bit]) can be selected.

- When [FREQUENCY] is set higher than 30p, the setting that can be selected will be restricted to [4K/10bit] and [UHD/10bit].

[MAIN CODEC] can be set to [OFF] when the V-RAW recorder is connected. It is also not possible to record in the main slot or sub slot when [HIGH SPEED] is set to [ON].

The Look file (.cdl/.vlt) linked to the clip will also be recorded with the same name as the V-RAW in accordance to the in-camera color grading function in the camera main unit.

NOTE

- UHD cannot be selected when [FREQUENCY] is set to 24p.

#### Recordable setting

[FREQUENCY] | [V-RAW] | [MAIN PIXEL] | [MAIN CODEC] | [SUB CODEC] | [HIGH SPEED]
--- | --- | --- | --- | --- | ---
Up to 30p | [4K/12bit] | [4096×2160] | [AVC-Intra4K 444] | [AVC-Intra422 & Pxy] [AVC-Intra100 & Pxy] [AVC-LongG50 & Pxy] [AVC-LongG25 & Pxy] | —
[2048×1080] | [AVC-Intra2K 444]
[4K/10bit] | [4096×2160] | [AVC-Intra4K 422]
[AVC-Intra4K-LT] | [OFF]/[ON]
[2048×1080] | [AVC-Intra2K 422]
[UHD/12bit] (excluding 24p) | [3840×2160] | [AVC-Intra4K 444] | —
[1920×1080] | [AVC-Intra444]
[UHD/10bit] (excluding 24p) | [3840×2160] | [AVC-Intra4K 422]
[AVC-Intra4K-LT] | [OFF]/[ON]
[1920×1080] | [AVC-Intra200] | —
[AVC-Intra422] | [OFF]/[ON]
[AVC-Intra100]
[ProRes 4444]
[ProRes 422 HQ]
Up to 60p | [4K/10bit] | [4096×2160] | [AVC-Intra4K 422] | —
[AVC-Intra4K-LT] | [OFF]/[ON]
[2048×1080] | [AVC-Intra2K 422]
[UHD/10bit] | [3840×2160] | [AVC-Intra4K 422] | —
[AVC-Intra4K-LT] | [OFF]/[ON]
[1920×1080] | [AVC-Intra422]
[AVC-Intra100]
[ProRes 422 HQ]

Top of the page