- Top
- Preparation
- Preparing the memory card
- Recording time of the memory card

# Recording time of the memory card

## When the recording mode is P2

SDHC memory cards, SDXC memory cards and microP2 cards can be used.

Recording format | Recording capacity
--- | ---
64 GB | 64 GB (during proxy recording)
AVC-Intra 422 AVC-Intra 200 AVC-Intra 100 (1080-59.94p/50.00p) | Approx. 32 minutes | Approx. 30 minutes
AVC-Intra 100 (1080-59.94i/50.00i, 720-59.94p/50.00p) | Approx. 64 minutes | Approx. 60 minutes
AVC-Intra 50 | Approx. 128 minutes | Approx. 114 minutes
AVC-LongG50 | Approx. 128 minutes | Approx. 114 minutes
AVC-LongG25 (1080-59.94p/50.00p) | Approx. 128 minutes | Approx. 114 minutes
AVC-LongG25 (1080-59.94i/50.00i, 720-59.94p/50.00p) | Approx. 256 minutes | Approx. 206 minutes
AVC-LongG12 (1080-59.94p/50.00p) | Approx. 240 minutes | —
AVC-LongG12 (1080-59.94i/50.00i, 720-59.94p/50.00p) | Approx. 480 minutes | —

NOTE

- For details on the SD card that the operation is confirmed, visit the support desk at the following website:

  https://pro-av.panasonic.net/

- The clip in P2 format data is split every 4 GB when [SPLIT] is selected in the [RECORDING] menu → [FILE SPLIT].

  Also, it is split approximately every 128 seconds if [SHORT SPLIT] is selected in the [RECORDING] menu → [FILE SPLIT].

  However, when recording to a memory card exceeding 32 GB in AVC-Intra 422/AVC-LongG50/AVC-LongG25/AVC-LongG12 formats, recording can be continued as a same clip by selecting [ONE FILE] in the [RECORDING] menu → [FILE SPLIT]. Clip is split approximately every three hours when recording format is AVC-Intra 422. Clip is split approximately every three hours or approximately every 64 GB when recording format is AVC-LongG50/AVC-LongG25/AVC-LongG12.

  These split clips are displayed as one clip in the thumbnail screen.

  These may be displayed as separate clips in the nonlinear editing software or a computer.

- The recording is stopped once when the recording time reaches ten hours, and recording is automatically resumed after few seconds. Image and audio during the pause will not be recorded. This includes the case of special recording, such as relay recording.

- In the interval recording, the recording is stopped once when the length of a clip reaches ten hours, and recording is automatically resumed after few seconds.

## When the recording mode is MOV

SDXC memory cards and 64 GB microP2 cards can be used. SDHC memory cards and 32 GB microP2 cards can not be used.

Recording format | Recording rate | Recording capacity
--- | --- | ---
64 GB | 128 GB
UHD | 400 Mbps | Approx. 20 minutes | Approx. 40 minutes
200 Mbps | Approx. 40 minutes | Approx. 1 hour 20 minutes
150 Mbps | Approx. 55 minutes | Approx. 1 hour 50 minutes
100 Mbps | Approx. 1 hour 20 minutes | Approx. 2 hours 40 minutes
FHD | 200 Mbps | Approx. 40 minutes | Approx. 1 hour 20 minutes
100 Mbps | Approx. 1 hour 20 minutes | Approx. 2 hours 40 minutes
50 Mbps | Approx. 2 hours 40 minutes | Approx. 5 hours 20 minutes

NOTE

- The recording time will change depending on the variable frame rate set in the variable frame rate recording or the super slow recording.

- File is split approximately every three hours for the data in MOV format.

  These are displayed as separate clips in the thumbnail screen. In addition, the clips recorded across two memory cards using the relay recording are displayed as separate clips.

- The recording is stopped once when the recording time reaches ten hours, and recording is automatically resumed after few seconds. Image and audio during the pause will not be recorded. This includes the case of special recording, such as variable frame rate recording, super slow recording or relay recording.

  When performing high-speed shooting with the variable frame rate recording or super slow recording, the recording time will be shorter than 10 hours depending on the ratio of the frame rate of the recording format and the variable frame rate.

- In the interval recording, the recording is stopped once when the length of a clip reaches ten hours, and recording is automatically resumed after few seconds.

## When the recording mode is AVCHD

SDHC memory cards, SDXC memory cards and microP2 cards can be used.

#### For SDHC memory card

Recording format | Recording rate | Recording capacity
--- | --- | ---
4 GB | 8 GB | 16 GB | 32 GB
PS | 25 Mbps | Approx. 19 minutes | Approx. 40 minutes | Approx. 1 hour 20 minutes | Approx. 2 hours 40 minutes
PH | 21 Mbps | Approx. 21 minutes | Approx. 46 minutes | Approx. 1 hour 30 minutes | Approx. 3 hours
HA | 17 Mbps | Approx. 30 minutes | Approx. 1 hour | Approx. 2 hours | Approx. 4 hours 10 minutes
PM | 8 Mbps | Approx. 1 hour | Approx. 2 hours | Approx. 4 hours 15 minutes | Approx. 8 hours 30 minutes
SA | 9 Mbps | Approx. 1 hour | Approx. 2 hours | Approx. 4 hours | Approx. 8 hours

#### For SDXC memory card

Recording format | Recording rate | Recording capacity
--- | --- | ---
64 GB | 128 GB
PS | 25 Mbps | Approx. 5 hours 20 minutes | Approx. 11 hours
PH | 21 Mbps | Approx. 6 hours | Approx. 12 hours 30 minutes
HA | 17 Mbps | Approx. 8 hours 30 minutes | Approx. 17 hours
PM | 8 Mbps | Approx. 17 hours 10 minutes | Approx. 35 hours
SA | 9 Mbps | Approx. 16 hours | Approx. 32 hours 15 minutes

NOTE

- File is split approximately every 4 GB for the data in AVCHD format.

  These are displayed as one clip in the thumbnail screen. However, the clips recorded across two memory cards using the relay recording are displayed as separate clips.

- The recording is stopped once when the recording time reaches ten hours, and recording is automatically resumed after few seconds. Image and audio during the pause will not be recorded. This includes the case of special recording, such as relay recording.

- Protection is automatically released on memory cards locked with AVCHD protection such as DVD recorders.

Top of the page