- Top
- Shooting
- Special recording function
- Shot mark recording function

# Shot mark recording function

Shot mark is a marker attached to the thumbnail of a clip to distinguish from other clips.

It is possible to display or play back only the clips with the shot mark.

## Adding shot mark

#### Assigning [SHOT MARK] to the USER button

Select the [CAMERA] menu → [USER SW] → [USER1] to [USER12] → [SHOT MARK].

#### Adding shot mark

Press the USER button with [SHOT MARK] assigned while recording or while paused after recording.

[MARK ON] is displayed in the camera image screen, and the shot mark is added to the clip that is recording. In case of paused after recording, the shot mark is added to the clip that was recorded immediately before.

[MARK OFF] is displayed and the shot mark is cleared by pressing again.

NOTE

- A shot mark can be added/cleared only on the clips in P2 format.

- A shot mark can also be added while displaying the thumbnail. (Adding shot mark to a clip)

- A shot mark cannot be added during recording in case of interval recording.

- A shot mark can only be added from the thumbnail display after recording in case of simultaneous recording.

- [SHOT MARK INVALID] is displayed when the USER button is pressed if the operation is invalid.

- Adding/clearing of the shot mark is not possible while playing back or paused during the playback.

- There are following restrictions when a shot mark is to be added/cleared for a linked clip such as a clip recorded across multiple memory cards, etc.

  - All the memory cards constructing the clip must be inserted into the card slots.

  - A shot mark is added only to the first clip of the linked clips.

Top of the page