- Top
- Preparation
- Mounting accessories
- Mounting the lens hood

# Mounting the lens hood

## Removing

Lens hood release button

While pressing the lens hood release button, turn the lens hood in the direction of the arrow to remove it.

## Mounting

Mounting mark

Mounting mark

Insert the lens hood into the camera.

- Align the mounting marks on the lens hood and camera.

Turn the lens hood clockwise.

- Turn until the lens clicks and locks into place.

## Opening and closing the lens cover

Use the lens cover open/close lever to open and close the lens cover.

Open the lens cover when shooting.

When not using the camera, close the lens cover in order to protect the lens.

NOTE

- Do not press the lens cover with force. Doing so may damage the lens and lens cover.

- The lens cover may not open and close or the lens hood may not mount depending on the various filters and MC protectors mounted to the front lens of the camera.

Top of the page