- Top
- Overview
- What you can do with this camera
- Recording to the memory card

# Recording to the memory card

Recording in following types is possible.

- P2 recording (P2 MXF compatible)

- UHD and FHD recording

  (4:2:0 (10-bit) MOV recording (HEVC)/4:2:0 (8-bit) MOV recording/4:2:2 (10-bit) MOV recording)

- AVCHD recording

- Variable frame rate recording

  (Supports 120fps/100fps shooting at the FHD resolution)

- Simultaneous recording

- Relay recording

- Interval recording

- Background recording

- Pre-recording

- 4ch audio recording

Top of the page