- Top
- Shooting
- Operation icon screen display
- Displaying the operation icon screen

# Displaying the operation icon screen

Press the multidial or the <SET> button while [ ICONS] is displayed in the LCD monitor, or touch the LCD monitor for one second or longer while the camera image screen is displayed.

- The operation icon screen is displayed.

  The camera returns to the camera image screen from the operation icon screen in the following cases.

  - When the <EXIT> button is pressed

  - When anything other than the icon is touched

  - When the touch operation of the LCD monitor and button operation of the <> button, <> button, <> button, </> button, or <SET> button are not performed for approximately five seconds

USER8

USER9

USER10

USER11

USER12

1. Scene file (1 to 6) icon

   Align the cursor and press the multidial or the <SET> button, or touch the icon to select each scene file.

   The name of each scene file is displayed on the second line of the icon.

2. [USER8] to [USER12] icon

   Align the cursor and press the multidial or the <SET> button, or touch the icon to execute the function assigned to [USER8] through [USER12].

   Each function assigned to [USER8] through [USER12] is displayed in the icon.

Top of the page