- Top
- Output and Screen Display
- Output format
- Format that can be output from the <HDMI> terminal

# Format that can be output from the <HDMI> terminal

The format that can be output from the <HDMI> terminal differs with following combination of the settings.

- [SYSTEM] menu → [FREQUENCY]

- [SYSTEM] menu → [REC FORMAT]

- [VIDEO OUT/LCD/VF] menu → [HDMI OUT] → [OUT FORMAT]

Item | Output format [OUT FORMAT]
--- | ---
[FREQUENCY] | [REC FORMAT]
Resolution | Frequency
[59.94Hz] | 3840×2160 | 59.94p | 3840×2160 59.94p 3840×2160 59.94p (4:2:0/8-bit) 1920×1080 59.94p (Factory setting) 1920×1080 59.94i
|  | 29.97p | 3840×2160 29.97p 1920×1080 29.97p (Factory setting)
|  | 23.98p | 3840×2160 23.98p 1920×1080 23.98p (Factory setting)
| 1920×1080 | 59.94p | 1920×1080 59.94p (Factory setting) 1920×1080 59.94i
|  | 59.94i | 1920×1080 59.94i
|  | 29.97p | 1920×1080 29.97p
|  | 23.98p | 1920×1080 23.98p
| 1280×720 | 59.94p | 1280×720 59.94p
| 720×480 | 59.94i | 720×480 59.94p
[50.00Hz] | 3840×2160 | 50.00p | 3840×2160 50.00p 3840×2160 50.00p (4:2:0/8-bit) 1920×1080 50.00p (Factory setting) 1920×1080 50.00i
|  | 25.00p | 3840×2160 25.00p 1920×1080 25.00p (Factory setting)
| 1920×1080 | 50.00p | 1920×1080 50.00p (Factory setting) 1920×1080 50.00i
|  | 50.00i | 1920×1080 50.00i
|  | 25.00p | 1920×1080 25.00p
| 1280×720 | 50.00p | 1280×720 50.00p
| 720×576 | 50.00i | 720×576 50.00p

NOTE

- The audio output from the <HDMI> terminal is two channels or four channels. The audio channel to output can be selected in the [AUDIO] menu → [OUTPUT SETTINGS] → [HDMI OUT CH].

- [OUT FORMAT] restores the factory settings when the settings of [FREQUENCY] and [REC FORMAT] change and the current setting values of [OUT FORMAT] cannot be acquired.

- The output format when playing back from the thumbnail screen is as follows.

  - It will be the value set in [OUT FORMAT] when the recording resolution of the playback clip is the same as [REC FORMAT].

  - It will be factory setting of [OUT FORMAT] when the recording resolution of the playback clip is different from [REC FORMAT].

Top of the page