- Top
- Shooting
- Multi manual function
- Setting the frame rate of the variable frame rate recording function

# Setting the frame rate of the variable frame rate recording function

Turn the multidial to display the [ FRAME RATE].

Press the multidial.

The frame rate display is highlighted in orange.

Turn the multidial to select the frame rate.

Press the multidial.

The setting changes to the value displayed and exits.

Press the <EXIT> button to exit without changing the setting.

When the REC button is pressed while it is possible to record, exits from the setting after changing the setting to the displayed value, and then the recording is started.

NOTE

- [ FRAME RATE] is displayed when the [SCENE FILE] menu → [VFR] → [ON] and the [SYSTEM] menu → [SUPER SLOW] → [OFF] are set.

Top of the page