- Top
- Preparation
- Assigning function to the USER buttons

# Assigning function to the USER buttons

<USER 1> button

<USER 2> button

<USER 3> button

<USER 4> button

<USER 5> button

<USER 6> button

<USER 7> button

Selected function can be assigned to the USER buttons.

The USER buttons have seven USER buttons on the camera (<USER 1> to <USER 7> buttons) and five USER button icons displayed on the LCD monitor ([USER8] to [USER12] button icons).

The <USER 1> to <USER 7> buttons can be used as the USER buttons when the camera image screen is displayed.

The [USER8] to [USER12] button icons can be used as the USER buttons when the operation icon screen is displayed.

Select the function to assign to each in the [CAMERA] menu → [USER SW] → [USER1] to [USER12].

#### Functions assigned to the USER buttons in the factory setting

USER button | Function
--- | ---
<USER 1> button | [O.I.S.]
<USER 2> button | [ZEBRA]
<USER 3> button | [WFM]
<USER 4> button | [A.IRIS LEVEL]
<USER 5> button | [SLOT SEL]
<USER 6> button | [IRIS]
<USER 7> button | [AWB]
[USER8] | [IR REC]
[USER9] | [FOCUS MACRO]
[USER10] | [AREA]
[USER11] | [ATW LOCK]
[USER12] | [MENU]

Functions assigned to USER buttons
Checking the function assigned to the USER buttons
Top of the page