- Top
- Shooting
- Variable frame rate (VFR) recording function/super slow recording function
- Super slow

# Super slow

This allows high-speed shooting of 120fps/100fps.

In the [SYSTEM] menu → [FREQUENCY]/[FILE FORMAT]/[REC FORMAT], select the resolution and codec for recording video and the frequency for the reference frame rate.

- For the combinations that can be set, refer to “Selecting the resolution, codec, and frame rate for recording video”.

Select the [SYSTEM] menu → [SUPER SLOW] → [ON].

- This can also be set even with the USER button.

  Refer to “Functions assigned to USER buttons”.

Press the REC button.

Super slow recording starts.

Top of the page