- Top
- Preparation
- Mounting accessories
- Mounting the external microphone

# Mounting the external microphone

External microphone such as the super-directional microphone AG-MC200G (optional) can be mounted onto the handle.

Screws are attached on the camera body in advance to protect the screw holes. Remove those screws when you attach the microphone holder.

- The microphone holder cannot be mounted with the screws originally attached to the camera. Use the supplied microphone holder screws.

Microphone holder screws

Microphone cable clamp

Microphone holder

<AUDIO INPUT 1> terminal

Fig. 1

Fig. 2

Fig. 3

Mount the supplied microphone holder to the microphone holder mounting section using the microphone holder screws (x 2). (Fig. 1)

Mount the external microphone and tighten the microphone holder screws. (Fig. 2)

Connect the microphone cable to the <AUDIO INPUT 1> terminal. (Fig. 3)

Attach the microphone cable to the microphone cable clamp.

Toggle the <INPUT1> switch to match the microphone to be connected.

NOTE

- Remove the microphone cable from the <AUDIO INPUT 1> terminal while pushing the lever.

Top of the page