- Top
- Shooting
- Convenient shooting functions
- Displaying frame marker

# Displaying frame marker

A frame marker can be displayed.

Select the angle of the view in the [VIDEO OUT/LCD/VF] menu → [MARKER] → [FRAME MARKER].

- The frame marker is not displayed when [OFF] is selected.

NOTE

- This is fixed to [OFF] when the [SYSTEM] menu → [REC FORMAT] → [480-59.94i/AVCHD SA]/[576-50.00i/AVCHD SA] and the [SYSTEM] menu → [ASPECT] → [4:3] are set.

## Setting the display color

Select the display color in the [VIDEO OUT/LCD/VF] menu → [MARKER] → [FRAME COLOR].

NOTE

- The marker cannot be recorded.

- The marker is not displayed while displaying the color bars when the enlarged display function of the focus assist function is enabled.

Top of the page