- Top
- Shooting
- Multi manual function

# Multi manual function

Operate the multidial to change settings and perform other operations without displaying the menu.

Operations can also be performed by pressing the </> button, <> button, <SET> button, and <EXIT> button.

You can execute the following functions.

Display of the camera image screen | Function
--- | ---
[ ICONS] | Displays the operation icon screen.
[ WB] | Sets the variable value for the white balance.
[ SHUTTER] | Sets the shutter speed.
[ SYNCHRO] | Sets the synchro scan shutter speed.
[ FRAME RATE] | Sets the frame rate of the variable frame rate recording function.
[ AREA] | Adjusts the area size/area position of the area mode function.
[ AF AREA] | Adjusts the width of the auto focus area.

Displaying the operation icon screen
Setting the variable value for the white balance
Setting the shutter speed
Setting the synchro scan shutter speed
Setting the frame rate of the variable frame rate recording function
Adjusting the area size/area position of the area mode function
Adjusting the width of the auto focus area
Top of the page