- Top
- Operation
- Handling setting data
- Scene files

# Scene files

## File structure of the setting data

The scene files of [F1:] to [F6:] can be saved in the camera memory in accordance to the scene file number.

What can be saved as a scene file is the setting contents of the [SCENE FILE] menu.

In addition, the current setting values of the scene files of [F1:] to [F6:] can be saved as a file to the camera memory and the memory card, and that data can be loaded and used in the camera.

Setting data file structure of the camera is as follows.

The camera

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

(Factory setting)

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

(Current value)

(Value saved on the camera)

[F2:]

[F3:]

[F5:]

[F1:]

[F4:]

Memory card

Scene file 1

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

Scene file n

[F1:]

[F2:]

[F3:]

[F4:]

[F5:]

[F6:]

[F6:]

[F6:]

[F6:]

[F6:]

The scene file can be initialized.

Select the [SCENE FILE] menu → [LOAD/SAVE/INITIALIZE] → [INITIALIZE].

Current setting value of each scene file can be individually saved in the camera body. Also, the scene files saved in the camera memory can be loaded.

Select the [SCENE FILE] menu → [LOAD/SAVE/INITIALIZE] → [LOAD]/[SAVE].

The scene file can be saved to the memory card in card slot 1. Also, the scene files saved in the memory card can be loaded.

## Saving the scene file

### Saving the scene file into the camera memory

Saves the current setting value of the camera into the camera memory.

Select the [SCENE FILE] menu → [LOAD/SAVE/INITIALIZE] → [SAVE].

### Saving the scene file to the memory card

The scene file can be overwritten to a file on the memory card in card slot 1, or saved as a new file.

#### Saving the scene file as a new file to the memory card

Specify a file name to save the current setting values of the camera to the memory card in card slot 1 as a new file.

Select the [OTHERS] menu → [FILE] → [SCENE FILE(SD CARD)] → [SAVE AS].

The file name entry screen and the keyboard are displayed.

Enter the text to set with the keyboard.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The file is saved.

- An error message may be displayed. For details about the error message, refer to “Cases indicated by error messages”.

#### Saving the scene file by overwriting a file on the memory card

Overwrite the file selected in the list of scene files saved in the memory card in card slot 1 with the current setting values of the camera.

Select the [OTHERS] menu → [FILE] → [SCENE FILE(SD CARD)] → [SAVE].

The list of scene files saved in the memory card in card slot 1 is displayed.

Select the file to overwrite from the list of scene files.

The file name entry screen and the keyboard are displayed. Leave it as is when overwriting.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The file is saved.

## Loading the scene file

Load the scene files saved to the camera memory or the memory card in card slot 1.

### Loading the scene file from the camera memory

Select the [SCENE FILE] menu → [LOAD/SAVE/INITIALIZE] → [LOAD].

### Loading the scene file from the memory card

Select the [OTHERS] menu → [FILE] → [SCENE FILE(SD CARD)] → [LOAD].

The list of scene files stored in the specified folder of the memory card in card slot 1 is displayed.

Select the file name for the file to load.

Selects if all of the scene files ([F1:] to [F6:]) are loaded, or individually loaded.

- To load all, select [ALL].

  To load individually, select the scene number to load.

Select [SET].

The file is loaded.

- An error message may be displayed. For details about the error message, refer to “Cases indicated by error messages”.

## Initialization of the scene file

Initializes the scene file saved in the camera memory.

Select the scene file to return to the factory setting in the [SCENE FILE] menu → [FILE SELECT].

Select the [SCENE FILE] menu → [LOAD/SAVE/INITIALIZE] → [INITIALIZE].

The confirmation screen is displayed.

Select [YES].

The selected scene file returns to the factory setting.

## Changing the scene file name

Changes the name of the scene file saved in the camera memory.

Only changeable part is the title section of the scene file name. As an example, if the scene file name is [F6:HLG], only the “HLG” part can be changed.

Select the scene file to change the name in the [SCENE FILE] menu → [FILE SELECT].

Select the [SCENE FILE] menu → [NAME EDIT].

The file name entry screen and the keyboard are displayed.

Enter the text to set with the keyboard. (Maximum eight characters)

Select [Enter].

The file name is updated.

Top of the page