- Top
- Connecting to External Devices
- Connecting with headphones and TV/monitor
- TV/monitor

# TV/monitor

A TV or monitor can be connected as shown in the following figure.

HDMI cable (optional)

BNC cable (optional)

TV/monitor

3.5 mm diameter video/audio cord 4-pole mini plug: Commercial product

Audio (Left audio: White)

Video (Yellow)

Ground

Audio (Right audio: Red)

NOTE

- VIERA Link is not supported on the camera. Note that the VIERA Link of other device may not properly operate when connected to the VIERA Link compatible device with a HDMI cable (optional).

- The SD resolution signal output from the <HDMI> terminal is output as a progressive signal (480P, 576P).

- For the BNC cable (optional) connected to the <SDI OUT> terminal, prepare a double-shielded cable equivalent to 5C-FB.

- Use the double shielded cable supporting 4K/60P as the HDMI cable (optional). Also, it is recommended to use the Panasonic HDMI cable compatible to 4K/60P as the HDMI cable.

Top of the page