- Top
- Network Connection
- Connecting to the iPhone/iPad or Android terminal
- Camera settings

# Camera settings

## Specifying the network settings

Specify the network settings. (Network settings)

## Setting the user account name and the password

Select the [NETWORK] menu → [IP REMOTE] → [USER ACCOUNT].

Enter the user account name and select [Enter].

- Enter the user account name with 31 characters or less.

Enter the password and select [Enter].

- Enter a password between 8 characters and 15 characters.

#### To enter a character

Operation is the same as entering with a keyboard.

Icon | Description of operation
--- | ---
[A-a] | Switches between upper case and lower case. (Displayed during the text entry mode)
[@-#] | Switches the type of the symbols. (Displayed during the symbol entry mode)
| Returns to the previous screen. Entered character is not reflected.
| Switches the character to symbol/number.
| Enters space (blank).
[BS] | Deletes the character. Previous character is deleted when the cursor position is empty.
/ | Moves the cursor to right or left.
[Enter] | Completes the character entry.

## Enabling the IP remote function

Select the [NETWORK] menu → [IP REMOTE] → [ENABLE/DISABLE] → [ENABLE].

## Checking/deleting user accounts

Select the [NETWORK] menu → [IP REMOTE] → [ACCOUNT LIST].

The list of registered user accounts is displayed.

- Proceed to Step 3 to only check user accounts.

Select the user account to delete, and then select [SET].

A confirmation message appears.

Select and end the operation.

Top of the page