- Top
- Specification
- Specifications
- AC adaptor

# AC adaptor

Power source AC 100 V – 240 V, 50 Hz/60 Hz, 1.2 A Power output DC 12 V, 3.0 A

indicates safety information.

Operating ambient temperature | 0 °C – 40 °C (32 °F – 104 °F)
Operating ambient humidity | 10% – 90% (relative humidity, no condensation)
Mass | Approx. 225 g (0.496 lbs.)
Dimensions (W×H×D) | 115 mm×37 mm×57 mm (4-1/2 inches × 1-7/16 inches × 2-1/4 inches) (excluding the DC cable section)

Top of the page