- Top
- Network Connection
- Connecting to the remote camera controller (AW-RP150G)
- Remote camera controller AW-RP150G setting

# Remote camera controller AW-RP150G setting

For details about the AW-RP150G setting, refer to the Operating Guide for the remote camera controller AW-RP150G.

NOTE

- Following information about the camera is required to connect to the AW-RP150G.

  - User account name

  - Password

  - IP address

  - Port No.: 49154

- For the firmware of the AW-RP150G, use Ver.4.01.00 or above.

- For details about the ROP setup software operation, refer to the Operating Instructions for the AW-RP150G.

- For ROP setup software, use Ver.3.0.0.0 or above.

Top of the page