- Top
- Preparation
- Preparing the memory card
- Inserting/removing the memory card

# Inserting/removing the memory card

## Inserting the memory card

The memory card to use with the camera should always be formatted on the camera. (Formatting the memory card)

- Formatting the memory card will erase all of the recorded data which cannot be restored.

Card 1 access lamp

Card slot 1

Card slot cover

Card slot 2

Card 2 access lamp

Open the card slot cover.

Insert the memory card into the card slot.

- Card slot 1 and card slot 2 can each insert one memory card.

- Insert straight in with the label facing left until it clicks.

  Do not force or apply excess force when inserting the memory card.

Close the card slot cover.

## Removing the memory card

Open the card slot cover.

- Confirm that the card access lamp is not flashing in orange.

- Data is being written/loaded when the card access lamp is flashing in orange, so do not remove the memory card.

Press in the memory card further into the camera and let go.

- Pull the memory card straight out when it is released from from the card slot.

Close the card slot cover.

## Cautions when using or storing

- Do not touch the connecting terminal section at the rear of the memory card.

- Avoid high temperature and humidity.

- Avoid water droplets.

- Avoid charging with electricity.

Use or store the memory card with the card inserted into the camera and with the slot cover closed.

Top of the page