- Top
- Preparation
- Memory cards
- Memory card recording time

# Memory card recording time

## When the recording mode is P2

Uses expressP2 card and microP2 card.

It is possible to record to SDXC memory cards in P2 format but is only for emergency recording and is not supported.

Recording format | Recording capacity
--- | ---
64 GB
AVC-Intra 422/AVC-Intra 200/AVC-Intra 100 (1080-59.94p/50.00p) | Approx. 32 minutes
AVC-Intra 100 (1080-59.94i/50.00i, 720-59.94p/50.00p) | Approx. 64 minutes
AVC-Intra 50 | Approx. 128 minutes
AVC-LongG50 | Approx. 128 minutes
AVC-LongG25 (1080-59.94p/50.00p) | Approx. 128 minutes
AVC-LongG25 (1080-59.94i/50.00i, 720-59.94p/50.00p) | Approx. 256 minutes
AVC-LongG12 (1080-59.94p/50.00p) | Approx. 240 minutes
AVC-LongG12 (1080-59.94i/50.00i, 720-59.94p/50.00p) | Approx. 480 minutes

NOTE

- Clip is split every 4 GB for the data in P2 format.

  However, when recording to a memory card exceeding 32 GB in AVC-Intra 422/AVC-LongG50/AVC-LongG25/AVC-LongG12 formats, recording can be continued as a same clip by selecting the [RECORDING] menu → [FILE SPLIT] → [ONE FILE]. Clip is split approximately every three hours when recording format is AVC-Intra 422. Clip is split approximately every three hours or approximately every 64 GB when recording format is AVC-LongG50/AVC-LongG25/AVC-LongG12.

  These split clips are displayed as one clip in the thumbnail screen.

  These may be displayed as separate clips in the nonlinear editing software or a computer.

- The recording is stopped once when the recording time reaches ten hours, and recording is automatically resumed after few seconds. Image and audio during the pause will not be recorded. This includes the case of special recording, such as relay recording.

- In the interval recording, the recording is stopped once when the length of a clip reaches ten hours, and recording is automatically resumed after few seconds.

- The camera does not support the CPS (Content Protection System) function of the P2 card, so a P2 card formatted with encryption with CPS password cannot be used. When formatted with the camera, it can be used as a P2 card that is not encrypted.

## When the recording mode is MOV

expressP2 card, 64 GB microP2 card, and SDXC card can be used. 32 GB microP2 card cannot be used.

Recording format | Recording rate | Recording capacity
--- | --- | ---
64 GB | 128 GB
UHD | 400 Mbps | Approx. 20 minutes | Approx. 40 minutes
200 Mbps | Approx. 40 minutes | Approx. 1 hour 20 minutes
150 Mbps | Approx. 55 minutes | Approx. 1 hour 50 minutes
100 Mbps | Approx. 1 hour 20 minutes | Approx. 2 hours 40 minutes
FHD | 200 Mbps | Approx. 40 minutes | Approx. 1 hour 20 minutes
100 Mbps | Approx. 1 hour 20 minutes | Approx. 2 hours 40 minutes
50 Mbps | Approx. 2 hours 40 minutes | Approx. 5 hours 20 minutes

NOTE

- File is split approximately every three hours for the data in MOV format.

  These are displayed as separate clips in the thumbnail screen. In addition, the clips recorded across two memory cards using the relay recording are displayed as separate clips.

- The recording is stopped once when the recording time reaches ten hours, and recording is automatically resumed after few seconds. Image and audio during the pause will not be recorded. This includes the case of special recording, such as relay recording.

- In the interval recording, the recording is stopped once when the length of a clip reaches ten hours, and recording is automatically resumed after few seconds.

Top of the page