- Top
- Operation
- Factory setting value of the scene file
- [SCENE FILE] menu

# [SCENE FILE] menu

Factory setting of each item in the scene file selected in the [SCENE FILE] menu → [FILE SELECT] are same values in [F1:] to [F6:].

- Meaning of the symbols used in the table are as follows.

  - —: Not a target.

[SCENE FILE] menu item | Factory setting
--- | ---
[FILE SELECT] | [F1:]
[SYNC SCAN TYPE] | [sec]
[SYNC SCAN] | [1/60.0]*1, [1/50.0]*2, [180.0d]*3
[MASTER DTL] | [0]
[DTL CORING] | [15]
[DETAIL SETTING]
[DETAIL] | [ON]
[H.DTL LEVEL] | [0]
[V.DTL LEVEL] | [0]
[DTL FREQ.] | [0]
[LEVEL DEPEND.] | [0]
[KNEE APE LEVEL] | [2]
[DTL GAIN(+)] | [0]
[DTL GAIN(−)] | [0]
[SKIN TONE DTL A] | [OFF]
[SKIN TONE DTL B] | [OFF]
[SKIN TONE DTL C] | [OFF]
[SKIN TONE ZEBRA] | [ON]
[SKIN TONE DTL SETTING]
[DETECT TABLE] | [A]
[SKIN DTL EFFECT] | [16]
[I CENTER] | [35]
[I WIDTH] | [2]
[Q WIDTH] | [2]
[Q PHASE] | [0]
[RB GAIN CONTROL SETTING]
[R GAIN AWB PRE] | [0]
[B GAIN AWB PRE] | [0]
[R GAIN AWB A] | [0]
[B GAIN AWB A] | [0]
[R GAIN AWB B] | [0]
[B GAIN AWB B] | [0]
[AWB A GAIN OFFSET] | [OFF]
[AWB B GAIN OFFSET] | [OFF]
[COLOR TEMP Ach SETTING]
[COLOR TEMP] | [3200K]
[R GAIN] | [0]
[B GAIN] | [0]
[G AXIS] | [0]
[COLOR TEMP Bch SETTING]
[COLOR TEMP] | [3200K]
[R GAIN] | [0]
[B GAIN] | [0]
[G AXIS] | [0]
[CHROMA LEVEL] | [0%]
[CHROMA PHASE] | [0]
[MATRIX]
[L MATRIX TABLE] | [A]
[M MATRIX TABLE] | [A]
[H MATRIX TABLE] | [A]
[MATRIX TABLE] | [A]
[ADAPTIVE MATRIX] | [OFF]
[R-G] | [0]
[R-B] | [0]
[G-R] | [0]
[G-B] | [0]
[B-R] | [0]
[B-G] | [0]
[COLOR CORRECTION]
[L COLOR CORRECT] | [ON]
[M COLOR CORRECT] | [ON]
[H COLOR CORRECT] | [ON]
16-axis independent color correction item [PARAMETER] | [0]
[MASTER PED] | [16]
[RGB BLACK CONTROL SETTING]
[R PED] | [0]
[G PED] | [0]
[B PED] | [0]
[PEDESTAL OFFSET] | [OFF]
[R FLARE] | [0]
[G FLARE] | [0]
[B FLARE] | [0]
[GAMMA MODE SEL] | [HD]
[GAMMA SETTING]
[MASTER GAMMA] | [0.45]
[F-REC DYNAMIC LEVEL] | [600%]
[F-REC BLACK STR LEVEL] | [0%]
[V-REC KNEE SLOPE] | [500%]
[V-REC KNEE POINT] | [30%]
[BLACK GAMMA] | [0]
[B.GAMMA RANGE] | [1]
[KNEE SETTING]
[MANUAL KNEE] | [ON]
[KNEE MASTER POINT] | [93.0%]
[KNEE MASTER SLOPE] | [99]
[A.KNEE POINT] | [90%]
[A.KNEE LEVEL] | [107]
[A.KNEE RESPONSE] | [4]
[HLG KNEE SW] | [OFF]
[HLG KNEE POINT] | [55]
[HLG KNEE SLOPE] | [10]
[HI-COLOR SW] | [ON]
[WHITE CLIP SETTING]
[WHITE CLIP] | [ON]
[WHITE CLIP LEVEL] | [109%]
[LOW SETTING]
[MASTER GAIN] | [0dB]
[H.DTL LEVEL] | [0]
[V.DTL LEVEL] | [0]
[DTL CORING] | [15]
[DTL FREQ.] | [0]
[LEVEL DEPEND.] | [0]
[MASTER GAMMA] | [0.45]
[BLACK GAMMA] | [0]
[B.GAMMA RANGE] | [1]
[MATRIX TABLE] | [A]
[COLOR CORRECT] | [ON]
[MID SETTING]
[MASTER GAIN] | [6dB]
[H.DTL LEVEL] | [0]
[V.DTL LEVEL] | [0]
[DTL CORING] | [15]
[DTL FREQ.] | [0]
[LEVEL DEPEND.] | [0]
[MASTER GAMMA] | [0.45]
[BLACK GAMMA] | [0]
[B.GAMMA RANGE] | [1]
[MATRIX TABLE] | [A]
[COLOR CORRECT] | [ON]
[HIGH SETTING]
[MASTER GAIN] | [12dB]
[H.DTL LEVEL] | [0]
[V.DTL LEVEL] | [0]
[DTL CORING] | [15]
[DTL FREQ.] | [0]
[LEVEL DEPEND.] | [0]
[MASTER GAMMA] | [0.55]
[BLACK GAMMA] | [0]
[B.GAMMA RANGE] | [1]
[MATRIX TABLE] | [A]
[COLOR CORRECT] | [ON]
[DRS] | [OFF]
[DRS EFFECT DEPTH] | [1]
[DNR] | [1]
[CAMERA SETTINGS]
[DETAIL] | [ON]
[GAMMA] | [ON]
[TEST SAW] | [OFF]
[FLARE] | [ON]
[H-F COMPE.] | [ON]

When the [SCENE FILE] menu → [SYNC SCAN TYPE] → [sec] is set, and the [SYSTEM] menu → [FREQUENCY] → [59.94Hz] is set

When the [SCENE FILE] menu → [SYNC SCAN TYPE] → [sec] is set, and the [SYSTEM] menu → [FREQUENCY] → [50.00Hz] is set

When the [SCENE FILE] menu → [SYNC SCAN TYPE] → [deg] is set

Top of the page