- Top
- Shooting
- Flash band compensation (FBC) function

# Flash band compensation (FBC) function

The camera is equipped with a function for compensating and reducing band-like interference (called “flash band”) that occurs due to the MOS pickup device when shooting in environments where flash strobe light such as that from still cameras is present.

Change over time

Flash firing

Shot image

Flash band

(FBC OFF)

Setting the flash band compensation function
Top of the page