- Top
- Overview
- When turning on the power for the first time
- [AREA SETTINGS]

# [AREA SETTINGS]

Set the region of use.

Connect the charged battery or the external DC power supply to the camera, and set the power switch to < > (ON).

The [AREA SETTINGS] screen is displayed.

Select the region of use.

[AREA 1]: Japan, Taiwan, South Korea

[AREA 2]: United States of America, Canada, Central and South America regions

[AREA 3]: Europe

[AREA 4]: Asia region (excluding Japan, Taiwan, South Korea), Oceania region, India

When the confirmation message is displayed, select [YES].

The camera will be initialized in accordance to the region selected in Step 2. The camera will automatically restart.

Once the setting for [AREA SETTINGS] is completed, the [TIME ZONE] screen is displayed.

NOTE

- Once this is set, the [AREA SETTINGS] screen is not displayed from the next startup.

- To change the region of use, set with the [OPTION] menu → [AREA SETTINGS].

#### Setting contents of each region of use

[RECORDING] → [REC MEDIA] is set to [microP2/SD].

Following setting differs depending on the selected region.

- The [SYSTEM] menu → [FREQUENCY]

- The [SYSTEM] menu → [REC FORMAT]

- The [OTHERS] menu → [CLOCK] → [DATE FORMAT]

- The [AUDIO] menu → [REC CH SETTINGS] → [HEAD ROOM]

- The [AUDIO] menu → [INPUT SETTINGS] → [REAR LINE IN LEVEL]

- The [AUDIO] menu → [OUTPUT SETTINGS] → [AUDIO OUT LEVEL]

- The [OTHERS] menu → [LANGUAGE]

Item | [AREA 1] | [AREA 2] | [AREA 3] | [AREA 4]
--- | --- | --- | --- | ---
[FREQUENCY] | [59.94Hz] | [59.94Hz] | [50.00Hz] | [50.00Hz]
[REC FORMAT] | [2160-59.94p/HEVC LongGOP 100M] | [2160-59.94p/HEVC LongGOP 100M] | [2160-50.00p/HEVC LongGOP 100M] | [2160-50.00p/HEVC LongGOP 100M]
[DATE FORMAT] | [Y-M-D] | [M-D-Y] | [D-M-Y] | [D-M-Y]
[HEAD ROOM] | [20dB] | [20dB] | [18dB] | [18dB]
[REAR LINE IN LEVEL] | [4dB] | [4dB] | [0dB] | [4dB]
[AUDIO OUT LEVEL] | [4dB] | [4dB] | [0dB] | [4dB]
[LANGUAGE] | [English] [] | [English] [Français] [Español] | [English] [Français] [Deutsch] [Español] [Italiano] | [English] [Français] [Español]

Top of the page