- Top
- Specification
- Specifications
- General

# General

Power DC 12 V (11.0 V – 17.0 V) Power consumption 32 W (body only, 2160-59.94p/HEVC LongGOP 100M standard recording status, LCD ON) 72 W (with all the accessories connected and maximum power supplied from each output terminal)

indicates safety information.

Operating ambient temperature | 0 °C – 40 °C (32 °F – 104 °F)
Operating ambient humidity | 10% – 85% (relative humidity)
Storage temperature | −20 °C – 60 °C (−4 °F – 140 °F)
Mass | Approx. 3.4 kg (7.5 lbs.) (body only)
Dimensions (W×H×D) | Body only 143 mm×267 mm×348 mm (5-5/8 inches × 10-1/2 inches × 13-23/32 inches) (excluding protrusion)

Top of the page