- Top
- Shooting
- Handling setting data
- Setup file

# Setup file

Specified menu can be saved or loaded to/from the camera memory or a SD card.

## Saving the setup file

Saves the current setting value of the camera into the camera memory or SD card.

[MENU]>[OTHERS]>[FILE]>[SETUP FILE(SD CARD)]>[SAVE AS]

[MENU]>[OTHERS]>[FILE]>[SETUP FILE(SD CARD)]>[SAVE]

[DEC-01-2019]

[DEC-01-2019]

[DEC-01-2019]

[DEC-01-2019]

Fig. 1

Fig. 2

### Saving a setup file as a new file on a SD card

Current setting values of the camera is saved as a new file in a SD card by specifying the file name.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(SD CARD)] → [SAVE AS].

The file name entry screen and the keyboard are displayed. (Fig. 1)

Enter the text to set with the keyboard.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The file is saved.

### Overwriting a setup file on SD card

Overwrites the file selected in the list of the setup files saved on the SD card with the current setting values of the camera.

Select [OTHERS] menu → [FILE] → [SETUP FILE(SD CARD)] → [SAVE].

The list of setup files saved on the SD card is displayed. (Fig. 2)

Select the file to overwrite from the list of setup files.

The file name entry screen and the keyboard are displayed. Leave it as is when overwriting.

Select [Enter].

A confirmation screen is displayed.

Select [SET].

The file is saved.

### Saving the setup file to the camera memory

Saves the current setting value of the camera into the camera memory.

Select [OTHERS] menu → [FILE] → [SETUP FILE(MEMORY)] → [SAVE].

## Loading the setup file

Loads a setup file from the camera memory or the SD card.

### Loading the setup file from the SD card

Loads a setup file saved in the SD card.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(SD CARD)] → [LOAD].

A list of setup files stored in the specified folder in the SD card is displayed.

Select the name of the file to load.

Select [SET].

Loading of the file is started. The camera is restarted after loading.

- An error message may be displayed. For error message, refer to “Warning system”.

- The file saved with different firmware version may not be able to load.

### Loading setup files from the camera memory

Loads the setup file saved on the camera memory.

Select the [OTHERS] menu → [FILE] → [SETUP FILE(MEMORY)] → [LOAD].

Loading of the file is started. The camera is restarted after loading.

Top of the page