- Top
- Preparation
- Preparing the memory card
- Memory cards supported on the camera

# Memory cards supported on the camera

Following expressP2 card, microP2 card, and SD card can be used with the camera. (As of December 2019)

Type of the expressP2 card | Recording capacity
--- | ---
expressP2 card A series | 256 GB
expressP2 card B series | 256 GB, 512 GB
expressP2 card C series | 256 GB, 512 GB

Type of the microP2 card | Recording capacity
--- | ---
microP2 card A series | 32 GB, 64 GB
microP2 card B series | 64 GB

- The camera does not support the CPS (Content Protection System) function of the P2 card, so a P2 card formatted with encryption with CPS password cannot be sued. When formatted with the camera, it can be used as a P2 card that is not encrypted.

Type of the SD card | Recording capacity
--- | ---
SDXC memory card | 48 GB - 128 GB

- The following memory cards cannot be used because they do not comply with the SD standards.

  - A memory card with 48 GB or more without the SDXC logo

- Operation is not guaranteed for any memory cards other than the above.

- Panasonic memory cards are recommended.

- Following memory cards cannot be used.

  - P2 memory card

  - microP2 card with microP2 card adaptor attached

## Speed Class during shooting

The type of the memory card to use differs depending on the recording mode and the recording format.

Use memory cards compatible with the Speed Class, UHS Speed Class, or Video Speed Class.

The recording may stop suddenly when a memory card not compatible with the required Speed Class is used.

- Speed Class, UHS Speed Class, and Video Speed Class are the speed specification regarding continuous writing. Check the display on the label and other information on the memory card.

#### When the recording mode is P2

Uses expressP2 card and microP2 card.

Recording bit rate or recording function | Type of memory card | Example of the logo display
--- | --- | ---
Memory card types supported on the camera | expressP2 card microP2 card |

#### When the recording mode is MOV

expressP2 card, 64 GB microP2 card, and SDXC card can be used.

SDHC card, 32 GB microP2 card cannot be used.

Recording bit rate or recording function | Type of memory card and Speed Class | Example of the logo display
--- | --- | ---
400 Mbps | Video Speed Class V60 or higher Or the expressP2 card, microP2 card B series |
200 Mbps | Video Speed Class V30 or higher, UHS Speed Class 3 or higher Or the expressP2 card, microP2 card |
150 Mbps
100 Mbps
50 Mbps | Video Speed Class V10 or higher, UHS Speed Class 1 or higher, Speed Class 10 or higher Or the expressP2 card, microP2 card |

Top of the page