- Top
- Connecting to External Devices
- Connecting with a recording device or a monitor

# Connecting with a recording device or a monitor

The camera directly controls the video and the monitor to output video.

Audio pin cable

Video equipment/monitor

HDMI cable

BNC cable (SDI)

NOTE

- VIERA Link is not supported on the camera. The VIERA Link of other device may not properly operate when connected to the VIERA Link compatible device with a HDMI cable (optional).

- The SD resolution signal output from the <HDMI> terminal is output as a progressive signal (480P, 576P).

- Use a double-shielded cable equivalent to 5C-FB for the BNC cable (optional) that is connected to the <SDI OUT1> terminal or the <SDI OUT2> terminal.

- Use the double-shielded cable supporting 4K/60p as the HDMI cable. Also, it is recommended to use the Panasonic HDMI cable supporting 4K/60p as the HDMI cable.

Top of the page